Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X

## R

REASON_IOSTREAM - Static variable in class com.alien.enterpriseRFID.notify.Message
REASON_TAGSTREAM - Static variable in class com.alien.enterpriseRFID.notify.Message
REPLY_BUFFER_SIZE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_DATA_SIZE_MISMATCH - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_DIAGNOSTIC_DATA - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_DIAGNOSTIC_END - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_DIAGNOSTIC_START - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_ERASE_FAILED - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_HARDWARE_ERROR - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_INVALID_KILL_CODE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_INVENTORY_END - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_INVENTORY_START - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_INVENTORY_TAG - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_KILL_FAILED - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LIST_DUMP_END - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LIST_DUMP_RECORD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LIST_DUMP_START - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LIST_FULL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LOCK_CRC_ERROR - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_LOCK_FAILED - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_MESSAGE_OK - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_MESSAGE_OK_G2 - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_NO_TAG - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_OVERFLOW_ERROR - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_PROGRAM_FAILED - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_RESUME - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_STRINGS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_SUSPEND - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_TAG_LOCKED - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_TAG_LOST - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UNKNOWN_COMMAND - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UNKNOWN_LENGTH - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UNKNOWN_TAG_COMMAND - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UNKNOWN_VALUE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UPLOAD_CRC_ERROR - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UPLOAD_END - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UPLOAD_INVALID - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UPLOAD_LINE_ERROR - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RESPONSE_UPLOAD_OK - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
RFMOD_DRM - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the "Dense Reader Mode" RFModulation.
RFMOD_HS - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the "High Speed" RFModulation.
RFMOD_STD - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the "Standard" RFModulation.
rc - Variable in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
rcCLI() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Enables raw DLE-based command sequences to be sent to the reader.
readXML() - Method in class com.alien.enterpriseRFID.util.XMLReader
  Scans the entire XML string, parsing its elements into a Hashtable.
readXML(Hashtable) - Method in class com.alien.enterpriseRFID.util.XMLReader
  Read entire XML into a given Hashtable.
readXMLNode(Hashtable) - Method in class com.alien.enterpriseRFID.util.XMLReader
  Reads and parses a single XML node into a Hashtable.
readerAdded(DiscoveryItem) - Method in interface com.alien.enterpriseRFID.discovery.DiscoveryListener
  A single reader has been added to the network.
readerCommandCLI() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Enables raw RQL-based command sequences to be sent to the reader.
readerCommandCLI() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Enables raw DLE-based command sequences to be sent to the reader.
readerRemoved(DiscoveryItem) - Method in interface com.alien.enterpriseRFID.discovery.DiscoveryListener
  A single reader has been removed from the network and is no longer available.
readerRenewed(DiscoveryItem) - Method in interface com.alien.enterpriseRFID.discovery.DiscoveryListener
  A single reader has renewed its lease.
reboot() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Causes the reader module to reboot.
reboot(boolean) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Reboots the reader, optionally waiting for the reader to finish booting before returning.
reboot() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Causes the reader module to reboot.
receiveBytes() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Receives and entire response message from the reader.
receiveBytes() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Receives and entire response message from the reader.
receiveLine() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Receives a line of string data from the reader.
receiveString(boolean) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Receives string data from the reader.
receiveString(boolean) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the response string prepared by the sendString() method, as it if came from a reader sporting an ASCII-based interface.
receiveString(boolean) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the response string prepared by the sendString() method, as it if came from a reader sporting an ASCII-based interface.
reformatTagID(String) - Static method in class com.alien.enterpriseRFID.util.Converters
  Converts a tagID string in a "nonstandard" format, to a format acceptable to a reader for programming operations.
removeOldTags() - Method in class com.alien.enterpriseRFID.tags.TagTable
  Removes Tags from this TagTable whose TimeToLive has reached zero.
removeTag(Tag) - Method in class com.alien.enterpriseRFID.tags.TagTable
  Removes a Tag from this TagTable.
replyBuffer - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyBufferRaw - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyCommType - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyCommTypeHexString - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyCommTypeMessage - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyLength - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyLengthRaw - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyValueHexArray - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyValueInt - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
replyValueIntArray - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
resetAutoMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. use #autoModeReset instead
resetBaudRate() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Attempts to set the serial communication baud rate of this reader to 115,200.
reverseBitArray(byte[]) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Reverses the order of a bit array.
run() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Reads heartbeat messages off the UDP port, and handle the data received.
run() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  This `SerialDiscoveryListenerService` will scan all the serial ports for Readers.
run() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Runs the MessageListenerService.
run() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Run the automode function for this reader.
run() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Run the automode function for this reader.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X