Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X

## S

SCANNING_END - Static variable in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Used to identify within an `ActionListener` that all of the ports have been scanned.
SCANNING_PORT - Static variable in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Used to identify within an `ActionListener` just what the action being reported is.
SCANNING_PORTBUSY - Static variable in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Used to identify within an `ActionListener` that a scanned port was busy.
SERIAL - Static variable in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Constant defining a "Serial" connection method.
SESSION_ID - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_AVAILABLE_BAUD_RATES - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_BIDIRECTIONAL_IO - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GENERAL_PURPOSE_INPUTS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GENERAL_PURPOSE_OUTPUTS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_AIR_INTERFACE_BAUD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_CAL_TABLE_ENTRY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_DECODE_PARAMETERS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_DIAGNOSTIC_MODE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_ETSI_LISTEN_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_HOP_TABLE_ENTRY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_MOD_CONTROL_MANUAL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_MOD_FUDGE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_NV_RAW - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_PA_BIAS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_PA_VDD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_PING_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_PROGRAM_LENGTH - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_PROGRAM_POWER_LEVELS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_RAW_MEMORY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_RAW_RF_POWER - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_RECEIVER_GAIN - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_SUSPENDERS_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_GET_TREE_INV_METHOD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_HOP_INTERVAL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_HOP_STEP_SIZE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_LOCALIZATION - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAXIMUM_ANTENNA_NUMBER - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAXIMUM_FREQUENCY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAXIMUM_HOP_TABLE_INDEX - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAXIMUM_RF_CHANNEL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAXIMUM_RF_POWER - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MAX_DIRECTED_SORT_LIST - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_MINIMUM_FREQUENCY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_OPERATING_VOLTAGE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_PLL_TYPE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_PROGRAMMER_ENABLE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_RADIO_TYPE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_READER_TYPE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_RESTORE_DEFAULT_HOP - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_RESTORE_DEFAULT_NV - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_RF_CHANNEL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SEND_MODULATION_CONT - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SEND_PRIMITIVE_ONE_SHOT - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_AIR_INTERFACE_BAUD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_CAL_TABLE_ENTRY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_DECODE_DIAG - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_DECODE_PARAMETERS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_DIAGNOSTIC_MODE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_ETSI_LISTEN_CHANNEL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_ETSI_LISTEN_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_HOP_TABLE_ENTRY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_MOD_CONTROL_MANUAL - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_MOD_FUDGE - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_NV_RAW - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_PA_BIAS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_PA_VDD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_PING_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_PROGRAM_LENGTH - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_PROGRAM_POWER_LEVELS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_RADIO_MANUF_INFO - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_RAW_MEMORY - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_RAW_RF_POWER - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_READER_MANUF_INFO - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_RECEIVER_GAIN - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_SUSPENDERS_PARAMS - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SET_TREE_INV_METHOD - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_SUPPORTED_TAG_TYPES - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SUBCMD_VOLTAGE_CALIBRATION - Static variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
SerialDiscoveryListenerService - class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService.
  `SerialDiscoveryListenerService` checks each serial port for a Reader.
SerialDiscoveryListenerService() - Constructor for class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Creates a new SerialDiscoveryListenerService.
SerialManager - class com.alien.enterpriseRFID.util.SerialManager.
  SerialManager in an interface to the javax.comm Serial routines.
SerialManager() - Constructor for class com.alien.enterpriseRFID.util.SerialManager
  Constructs a SerialManager object.
saveSettings() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Saves the current reader setting to flash memory.
sendBytes(byte[]) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sends an arbitrary sequence of bytes to the reader.
sendBytes(byte[]) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sends an arbitrary sequence of bytes to the reader.
sendString(String) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Sends string data to the reader.
sendString(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Intercepts a command string intended for the RQL-based reader, and attempts to handle the command using methods from this class.
sendString(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Intercepts a command string intended for the OEM reader, and attempts to handle the command using methods from this class.
sessionID - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
setAcqC1Mask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setAcqC1Mask(int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setAcqG2AccessPwd(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the Access password that the reader will use to gain access to password-protected portions of Class1/Gen2 tag memory.
setAcqG2Mask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the Class1/Gen2 mask, as a String.
setAcqG2Mask(int, int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the Class1/Gen2 Mask, specifying individual values.
setAcqG2MaskAction(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the include/exclude behavior of the Class1/Gen2 mask.
setAcqG2MaskAntenna(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the current value of AcqG2MaskAntenna.
setAcqG2SL(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the value of AcqG2SL, using a String.
setAcqMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setAcqMask(int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setAcquireC0Count(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of reads to perform in each Class0 acquire cycle.
setAcquireC0Cycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of complete acquire cycles to perform with each Class0 read operation.
setAcquireC1Count(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as setAcquireCount().
setAcquireC1Count(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of reads to perform in each C1 acquire cycle.
setAcquireC1Cycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as setAcquireCycles().
setAcquireC1Cycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of complete acquire cycles to perform with each C1 read operation.
setAcquireC1EnterWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as setAcquireEnterWakeCount().
setAcquireC1EnterWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of wakes to perform at the start of each C1 acquire cycle.
setAcquireC1ExitWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as setAcquireExitWakeCount().
setAcquireC1ExitWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of wakes to perform at the end each C1 acquire cycle.
setAcquireC1SleepCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as setAcquireSleepCount().
setAcquireC1SleepCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of sleeps to perform during each C1 acquire cycle.
setAcquireCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of reads to perform in each Class1 Gen1 acquire cycle.
setAcquireCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setAcquireCycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of complete acquire cycles to perform with each Class1 Gen1 read operation.
setAcquireCycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setAcquireEnterWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of wakes to perform at the start of each Class1 Gen1 acquire cycle.
setAcquireEnterWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setAcquireExitWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of wakes to perform at the end all the Class1 Gen1 acquire cycles.
setAcquireExitWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setAcquireG2Count(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of reads to perform in each Class1 Gen2 acquire cycle.
setAcquireG2Count(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of reads to perform in each G2 acquire cycle.
setAcquireG2Cycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of complete acquire cycles to perform with each Class1 Gen2 read operation.
setAcquireG2Cycles(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the number of complete acquire cycles to perform with each G2 read operation.
setAcquireG2Ops(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
setAcquireG2Ops(int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
setAcquireG2Ops(int, String, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
setAcquireG2OpsMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of AcqG2OpsMode.
setAcquireG2Q(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the starting Q value to use in each Class1 Gen2 acquire cycle.
setAcquireG2Q(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the starting Q value for each G2 acquire cycle.
setAcquireG2Selects(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of SELECT commands issued at the start of each Class1/Gen2 acquire cycle.
setAcquireG2Session(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the G2 Session that the reader will operate on when inventorying Class1/Gen2 tags.
setAcquireG2TagData(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies which additional locations in G2 tag memory to fetch in the course of an inventory.
setAcquireG2TagData(int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies a single additional location in G2 tag memory to fetch in the course of an inventory.
setAcquireG2Target(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the manner in which the reader manages the population of inventoried G2 tags.
setAcquireMode(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Specifies the method the reader uses to scan for tags.
setAcquireMode(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the method the reader uses to scan for tags.
setAcquireMode(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Specifies the method the reader uses to scan for tags.
setAcquireSleep(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF AcquireSleep setting.
setAcquireSleepCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of sleeps to perform during each Class1 Gen1 acquire cycle.
setAcquireSleepCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setAcquireTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the maximum inventory duration, after which the reader aborts the inventory.
setAcquireWakeCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes how often the reader performs automatic Wakes.
setActionListener(ActionListener) - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Registers an object with this `SerialDiscoveryListenerService` to receive messages about the progress of the serial port scanning.
setActiveAntenna(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sets the active antenna to the specified value.
setActiveAntenna(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the active antenna to the specified value.
setAddress(String, int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Set the address for this reader.
setAntenna(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the antenna that this Tag was last seen with.
setAntennaSequence(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sets the sequence of antenna ports, using a comma-separated String of integer values, that is used by the reader when responding to an Inventory command.
setAntennaSequence(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Change the sequence of antenna ports the reader cycles through as it performs reads.
setAntennaSequence(int[]) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the sequence of antenna ports, using an array of ints, that is used by the reader when responding to an Inventory command.
setAntennaSequence(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the sequence of antenna ports, using a comma-separated String of integer values, that is used by the reader when responding to an Inventory command.
setAutoAction(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the action the reader performs while in autonomous mode.
setAutoErrorOutput(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader setting specifying which AutoMode errors to react to, and the external output setting to apply when one of those errors is encountered.
setAutoFalseOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the value of the external output pins while in the "false pause" state.
setAutoFalsePause(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader pauses after the autonomous mode evaluation returns a `false` condition.
setAutoMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sets the ON/OFF status of Autonomous mode.
setAutoMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of Autonomous mode.
setAutoMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the ON/OFF status of Autonomous mode.
setAutoProgError(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader pauses after the autonomous mode evaluation returns a `false` condition.
setAutoStartPause(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader pauses after receiving a start trigger before it actually enters the work state.
setAutoStartTrigger(int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the external input pins the reader monitors that trigger autonomous mode to jump into the working state.
setAutoStartTrigger(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the external input pins the reader monitors that trigger autonomous mode to jump into the working state, as a comma-separated string.
setAutoStopPause(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader pauses after receiving a stop trigger before it actually leaves the work state.
setAutoStopTimer(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader spends in the work state before moving on to the evaluate state.
setAutoStopTrigger(int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the external input pins the reader monitors that trigger autonomous mode to leave the working state.
setAutoStopTrigger(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the external input pins the reader monitors that trigger autonomous mode to leave the working state, as a comma-separated string.
setAutoTrueOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the value of the external output pins while in the "true pause" state.
setAutoTruePause(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time the reader pauses after the autonomous mode evaluation returns a `true` condition.
setAutoWaitOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specify the value of the external output pins while in the wait state.
setAutoWorkOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the value of the external output pins while in the work state.
setBank(int) - Method in class com.alien.enterpriseRFID.reader.TagMemory
setBaudRate(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the reader's serial communication baud rate to the value specified.
setBidirectionalDDR(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the input/output direction of Bi-Directional I/O ports.
setC1MaskBits(int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setC1TagMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setCRC(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the CRC of this Tag's TagID.
setCommandPort(int) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Sets the port number that this DiscoveryItem's reader uses to accept and respond to host commands over the network.
setCommandPort(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Sets the port number that this DiscoveryItem's reader uses to accept and respond to host commands over the network.
setCommandPort(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the port that this reader listens on for command messages.
setConnection(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Sets this DiscoveryItem's connection method.
setConnection(String) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Specifies a reader's connection method, given as a single string.
setConnection(String, int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Sets a reader's connection method to TCP/IP, specifying both address and port.
setCustomFormatString(String) - Static method in class com.alien.enterpriseRFID.tags.TagUtil
setDHCP(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of DHCP.
setDNS(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the Domain Name Server for this reader.
setData(String) - Method in class com.alien.enterpriseRFID.reader.TagMemory
setDate(Date) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the Date for this Message.
setDebug(boolean) - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Sets the internal debug flag for this `MessageListenerService`.
setDebugLevel(int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Sets the current Debug Level.
setDebugLevel(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
setDebugLevel(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setDefaultIOListFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the IOListFormat to it's default setting, TEXT_FORMAT.
setDefaultTagListFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the tag list format to it's default setting, TEXT_FORMAT.
setDirection(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the apparent direction of the tag, toward or away from the antenna.
setDiscoverTime(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the discovery time of this Tag, as reported by the reader.
setDiscoveryListener(DiscoveryListener) - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Registers an object with this `NetworkDiscoveryListenerService` to receive messages when readers are discovered, renewed, or removed from the network.
setDiscoveryListener(DiscoveryListener) - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Registers an object with this `SerialDiscoveryListenerService` to receive messages when readers are discovered, renewed, or removed on the serial ports.
setDiscoveryMethod(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Specifies the method with which this DiscoveryItem's reader was discovered.
setEventTime(long) - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets the timestamp of this ExternalIO event, as reported by the reader's on-board clock.
setEventTimeHost(long) - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets the timestamp of this ExternalIO event, as reported by the host system's clock.
setEventTimeHost() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets the timestamp of this ExternalIO event, as reported by the host system's clock, to the current system time.
setExternalOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the state of the reader's external output pins.
setExternalOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Changes the state of the reader's external output pins.
setFactorySettings() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Resets the reader to its original factory settings, and waits for it to reboot.
setFactorySettings(boolean) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Resets the reader to its original factory settings, and optional waits for it to reboot.
setFirstHeartbeat(long) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Specifies the time that this DiscoveryItem first registered a heartbeat signal from its reader.
setG2Data(int, String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Stores a chunk of additional Gen2 tag data, as a String.
setG2Mask(int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setG2MaskBits(int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the Class1/Gen2 Mask, specifying individual bit values.
setG2Ops(int, String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Stores a result from a specific G2Ops action.
setG2TagMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's Class1/Gen2 tag mask to match the specified EPC.
setG2TagMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
setGateway(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the IP address of the network Gateway server.
setHashtable(Hashtable) - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Sets the Hashtable that this XMLWriter uses to generate its XML document.
setHeartbeatAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the IP address where reader heartbeat messages are delivered.
setHeartbeatCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the number of heartbeat messages that the reader will broadcast following startup.
setHeartbeatPort(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the port number over which the reader sends its UDP heartbeat messages.
setHeartbeatTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the time interval between heartbeat messages.
setHostDiscoverTime(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the discovery time of this Tag, as reported by the host.
setHostRenewTime(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the time this Tag was last seen, as reported by the host.
setHostname(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the network hostname for this reader.
setIOList(ExternalIO[]) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the IOList of this `Message` as an array of `ExternalIO`s.
setIOListCustomFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the custom IOList formatting string.
setIOListFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the type of format to use for IOLists.
setIOPortValue(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets or clears specified output port pins.
setIOStreamAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the address of the device to push IOStream events to.
setIOStreamAddress(String, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the address of the device to push IOStream events to.
setIOStreamCustomFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the custom IOStream formatting string.
setIOStreamFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of format used for IOStream event messages.
setIOStreamKeepAliveTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the time period (in seconds) the reader will hold an idle IOStream TCP socket open before closing it.
setIOStreamMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of the reader's IOStream functionality.
setIOType(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the type of external I/Os that the reader will report from its internal IOList.
setIPAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes this reader's network IP Address.
setIndentSize(int) - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Sets the number of space characters used to indent each level of XML output.
setInitExternalOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the value used to set the external output state during startup.
setInputStream(InputStream) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Set the InputStream as a InputStream
setInputStream(InputStream) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the InputStream object for the serial port managed by this SerialManager.
setInvertExternalInput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of the external input inverter.
setInvertExternalOutput(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of the external output inverter.
setIsCustomTagList(boolean) - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Sets the flag indicating whether this `MessageListenerService` should use the custom taglist decoder, or the standard "Text" format decoder.
setLBT(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of LBT.
setLBTLimit(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the value for the LBT threshold.
setLastHeartbeat(long) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Specifies the time that this DiscoveryItem last registered a heartbeat signal from its reader.
setLeaseTime(int) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Sets the amount of time that this DiscoveryItem's reader waits between sending heartbeat messages across the network.
setLeaseTime(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Sets the amount of time that this DiscoveryItem's reader waits between sending heartbeat messages across the network.
setLen(int) - Method in class com.alien.enterpriseRFID.reader.TagMemory
setLineTerminator(String) - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Sets the line terminator string that this XMLWriter uses to end each of the lines of its XML output.
setListenerInterface(InetAddress) - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Specifies the interface IP address for this `MessageListenerService` to listen on for reader notification messages.
setListenerPort(int) - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Sets the port number for this service to listen on.
setListenerPort(int) - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Specifies the port number for this `MessageListenerService` to listen on for reader notification messages.
setLogLevel(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
setLogging(String, boolean) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Enables or disables logging for a specified tag.
setLoggingInterval(String, byte[]) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Sets the periodicity at which the tag logs sensor data to tag memory, with timing values specified as a triple byte array.
setLoggingInterval(String, int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Sets the periodicity at which the tag logs sensor data to tag memory, with timing values specified as individual integers.
setMailFrom(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the email address associated with this reader.
setMailServer(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the SMTP (Simple Mail Transfer Protocol) mail server.
setMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setMask(int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setMask(int, int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Set the Tag Mask, using a length, pointer, and string of hex bytes as parameters.
setMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the Tag Mask, as a String.
setMaskBits(int, String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
setMaxSerialPort(int) - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Deprecated. use `SerialDiscoveryListenerService.setSerialPortList(String)` instead
setMemory(String, int, byte[]) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Stores a series of bytes into tag memory.
setMemoryPacketSize(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Specifies the number of bytes to use in each memory related transmission packet to and from the tag.
setMessageListener(MessageListener) - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Registers a `MessageListener` with this `MessageListenerService` to be notified when a new notification message is received from a reader.
setMyData(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the arbitrary "MyData" stored on the reader.
setNetmask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the netmask of this reader.
setNetworkConnection(String, int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Specifies the IP Address and Command Channel Port for this reader.
setNetworkTimeout(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the time period (in seconds) the reader will wait on an idle network connection before timing out.
setNetworkUpgrade(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of the network upgrade flag.
setNotifyAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the address (as a single String) of the device to push notifications to.
setNotifyAddress(String, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the address (as IP and port number) of the device to push notifications to.
setNotifyFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the type of format used for notification messages.
setNotifyHeader(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of NotifyHeader.
setNotifyInclude(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the value indicating whether Tag data, I/O data, or both will be included in Notification messages.
setNotifyKeepAliveTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the time period (in seconds) the reader will hold an idle Notify TCP socket open before closing it.
setNotifyMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of Notify mode.
setNotifyQueueLimit(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Serts the total number of failed TCP notification messages that the reader will queue up, waiting for the connection to the NotifyAddress to be reestablished.
setNotifyRetryCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the number of times the reader should retry a notification message that failed to be delivered, before turning NotifyMode off.
setNotifyRetryPause(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the amount of time (in seconds) that the reader should retry wait before reattempting a failed notification message.
setNotifyTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the time interval for automatic pushing of tag lists.
setNotifyTrigger(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the event conditions (other than time-based) upon which a notification message is sent out to any listener.
setOutputStream(OutputStream) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Set the OutputStream as a OutputStream
setOutputStream(OutputStream) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the OutputStream object for the serial port managed by this SerialManager.
setPCWord(String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Stores information about a tag's Protocol Control (PC) information.
setPassword(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Specifies the password associated with this DiscoveryItem's reader.
setPassword(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Change the password this `AlienClass1Reader` uses to authenticate with the reader over the network.
setPersistTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sets the time, in seconds, that tags on the internal TagList will persist without having been read, before being purged from the list.
setPersistTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the length of time a tag's data will remain in the reader's internal list of active tags.
setPersistTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the time, in seconds, that tags on the internal TagList will persist without having been read, before being purged from the list.
setPersistTime(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the PersistTime associated with this Tag.
setPersistTime(int) - Method in class com.alien.enterpriseRFID.tags.TagTable
  Specifies the persistence time for tags in this TagTable.
setProgAlienImageMap(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Set the memory map specifier used by the ProgramAlienImage command.
setProgAlienImageNSI(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the NSI data that the reader will write to the tag during the next ProgramAlienImage.
setProgAntenna(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Sets the programming antenna to the specified value.
setProgAntenna(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the antenna that the reader uses for programming operations.
setProgAntenna(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the programming antenna to the specified value.
setProgAttempts(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the number of times the reader attempts to program a tag.
setProgBlockAlign(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the new ON/OFF value for ProgBlockAlign.
setProgBlockSize(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the new ProgBlockSize value.
setProgC1KillPwd(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the kill password that the reader will use to lock or kill the next Class 1, Gen 1 tag, while operating in AutoMode.
setProgDataUnit(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the size of the data unit used to read and write to Gen2 tags.
setProgEPCData(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the EPC data reader will use to program the next tag in AutoMode, or when the ProgramEPC command is issued without a corresponding EPC data argument.
setProgEPCDataInc(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the programming result that triggers the ProgEPCData property of the reader to be incremented.
setProgEPCDataIncCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum number of times the reader will automatically increment the ProgEPCData value before prohibiting further programming operations.
setProgEraseAttempts(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the number of times the reader attempts to erase a tag, before programming it.
setProgG2AccessPwd(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the Access Password that the reader will use when the ProgramAccessPwd command is issued without a corresponding data argument.
setProgG2KillPwd(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the kill password that the reader will use to lock or kill the next Class 1, Gen 2 tag, while operating in AutoMode.
setProgG2LockType(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the type of lock used to lock the next Class1/Gen2 tag.
setProgG2NSI(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the NSI data that the reader will write to the tag during the next ProgramEPC operation.
setProgIncrementOnFail(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the ON/OFF status of the ProgIncrementOnFail flag.
setProgProtocol(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the tag protocol that the reader uses for programming operations.
setProgReadAttempts(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the number of times the reader attempts to verify the presence of a tag, before programming it .
setProgSingulate(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of whether the reader will try to singulate a tag before programming it.
setProgUserData(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the USER data that the reader will use when the ProgramUser command is issued without a corresponding data argument.
setProgUserDataInc(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the programming result that triggers the ProgUserData property of the reader to be incremented.
setProgUserDataIncCount(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum number of times the reader will automatically increment the ProgUserData value before prohibiting further programming operations.
setProgramID(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the tagID the reader will use to program the next tag in AutoMode.
setProgramPassCode(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the PassCode the reader will use to lock or kill the next tag, while in AutoMode.
setProtocol(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the protocol code.
setProtocol(String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the protocol string for this tag.
setPtr(int) - Method in class com.alien.enterpriseRFID.reader.TagMemory
setRFAttenuation(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFAttenuation value.
setRFAttenuation(int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFAttenuation value for a specific antenna.
setRFAttenuation(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the RF power attenuation to the value associated with argument provided.
setRFAttenuations(int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFAttenuation values for a specific antenna, with different values for reading and writing operations.
setRFLevel(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFLevel value.
setRFLevel(int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFLevel value for a specific antenna.
setRFLevels(int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's RFLevel value for a specific antenna, with different values for reading and writing operations.
setRFModulation(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's current Class 1 Gen2 modulation mode.
setRFOnOff(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Turns the RF carrier on or off while idle (not reading tags).
setRSSI(double) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets this tag's Return Signal Strength Indication.
setRSSIFilter(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the String defining the current RSSIFilter ranges.
setRSSIFilter(float, float) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the String defining the current RSSIFilter ranges.
setRawData(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the raw content of this Message.
setReaderAddress(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Changes the reader address of this DiscoveryItem.
setReaderBaudRate(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's current serial baud rate.
setReaderCommandPort(int) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the ReaderCommandPort value for this Message.
setReaderFunction(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's current operating mode.
setReaderHostname(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the network hostname value for this Message.
setReaderIPAddress(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the IPAddress value for this Message.
setReaderMACAddress(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Changes the reader MAC address of this DiscoveryItem.
setReaderMACAddress(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the MACAddress value for this Message.
setReaderName(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Changes this DiscoveryItem's ReaderName value.
setReaderName(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the ReaderName value for this Message.
setReaderName(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the reader's Name.
setReaderNumber(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's numerical identifier.
setReaderNumber(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Changes the ReaderNumber parameter of this reader.
setReaderPassword(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the actual password stored in the reader.
setReaderType(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Changes this DiscoveryItem's ReaderType value.
setReaderType(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the ReaderType value for this Message.
setReaderUsername(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the actual username stored in the reader.
setReaderVersion(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Changes this DiscoveryItem's ReaderVersion value.
setReason(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the Reason value for this Message.
setReceiveAntenna(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the receive antenna that this Tag was last seen with.
setRenewCount(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the number of times this Tag has been read.
setRenewTime(long) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the time this Tag was last seen by the reader.
setSerialBaudRate(int) - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Sets the hserial baud rate used to discover serially-connected readers.
setSerialBaudRate(int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Tells the Serial Manager to communicate with the reader at a specified baud rate.
setSerialBaudRate(int) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the communication rate of the serial port managed by this SerialManager.
setSerialConnection(String) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Use the serial port given by `serialPortName` to communicate with this reader.
setSerialPort(SerialPort) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the SerialPort object managed by this SerialManager.
setSerialPortList(String) - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Specifies which serial ports will be scanned.
setSerialPortName(String) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the name of the serial port managed by this SerialManager.
setSerialPortTimeout(int) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Sets the communication timeout value for the serial port managed by this SerialManager.
setSpeed(double) - Method in class com.alien.enterpriseRFID.tags.Tag
  Updates this Tag's speed measurement.
setSpeedFilter(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the String defining the current SpeedFilter ranges.
setSpeedFilter(float, float) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the String defining the current SpeedFilter ranges.
setSpeedSmoothingCoefficient(double) - Static method in class com.alien.enterpriseRFID.tags.Tag
  Sets the current speed smoothing coeefficient.
setStartTriggerLines(int) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the external input lines that triggered this autonomous cycle to start.
setStopTriggerLines(int) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the external input lines that triggered this autonomous cycle to stop.
setStreamHeader(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of StreamHeader.
setSupportedTagTypes(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the bitmap indicating which Alien RFID tag types the reader should look for.
setTagAuth(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the TagAuth setting on the reader.
setTagAuth(String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Stores information about tag authentication.
setTagID(String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the value of this Tag's TagID attribute.
setTagList(Tag[]) - Method in class com.alien.enterpriseRFID.notify.Message
  Sets the TagList of this `Message` as an array of `Tag`s.
setTagListAntennaCombine(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of the TagList Antenna Combine feature.
setTagListCustomFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the custom tag list formatting string.
setTagListFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the type of format to use for tag lists.
setTagListMillis(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of the TagList Milliseconds feature.
setTagMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the reader's tag mask to match the specified Tag ID.
setTagMask(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Sets the reader's tag mask to match the specified Tag ID.
setTagStreamAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the address of the device to push TagStream events to.
setTagStreamAddress(String, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the address of the device to push TagStream events to.
setTagStreamCountFilter(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the minimum number of times a given tag has to be read before the reader will start streaming that tag data.
setTagStreamCountFilter(int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the minimum number of times a given tag has to be read before the reader will start streaming that tag data.
setTagStreamCustomFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the custom TagStream formatting string.
setTagStreamFormat(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of format used for TagStream event messages.
setTagStreamKeepAliveTime(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the time period (in seconds) the reader will hold an idle TagStream TCP socket open before closing it.
setTagStreamMode(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the ON/OFF status of the reader's TagStream functionality.
setTagTableListener(TagTableListener) - Method in class com.alien.enterpriseRFID.tags.TagTable
  Registers a `TagTableListener` with this TagTable to be notified when the tag list changes.
setTagType(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
setTagType(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the bitmap indicating which Alien RFID tag types the reader should look for.
setTime(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the date and time of the reader's onboard clock.
setTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the date and time of the reader's onboard clock to the host's current values.
setTime(Date) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the date and time of the reader's onboard clock.
setTimeOutMilliseconds(int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Sets the maximum time to wait for a reader's reply before giving up.
setTimeOutMode(int) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
setTimeServer(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies the address of the external TimeServer the reader uses to accurately set its internal clock each time it is rebooted.
setTimeZone(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the reader's time zone setting.
setTopLevelTag(String) - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Sets the top-level tag string that this XML writer wraps around its XML output.
setTransmitAntenna(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Sets the transmit antenna that this Tag was last seen with.
setType(int) - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets this ExternalIO's type.
setType(String) - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets this ExternalIO's type, given as a String, "DI" or "DO".
setUpgradeAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the URL where the reader will look for upgrade files.
setUpgradeIPAddress(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the IP address for the Reader Upgrade Service (RUS) where the reader will look for upgrade files.
setUpgradePort(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Changes the port number for the Reader Upgrade Service (RUS) that the reader will connect to when it looks for upgrades over the network.
setUsername(String) - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Specifies the username associated with this DiscoveryItem's reader.
setUsername(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Change the username this `AlienClass1Reader` uses to authenticate with the reader over the network.
setValidateOpen(boolean) - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Specify if the reader should be validated every time it is opened for communications.
setValue(int) - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Sets the value for this ExternalIO.
setValue(byte[], long, int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Inserts values into an existing bit array.
setWWWPort(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Sets the port number that the reader's built-in web server listens on.
setXML(String) - Method in class com.alien.enterpriseRFID.notify.Message
  Deprecated. Use `Message.setRawData(String)` instead.
setXMLString(String) - Method in class com.alien.enterpriseRFID.util.XMLReader
  Sets the XML string to be parsed.
setXPC(String) - Method in class com.alien.enterpriseRFID.tags.Tag
  Stores information about a tag's Extended Protocol Control (XPC) information.
setZeroSpeedThresholdHigh(double) - Static method in class com.alien.enterpriseRFID.tags.Tag
  Sets the high end of the zero-speed threshold range.
setZeroSpeedThresholdLow(double) - Static method in class com.alien.enterpriseRFID.tags.Tag
  Sets the low end of the zero-speed threshold range.
sleep(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. use sleepTag() instead
sleepTag(String) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Requests all tags in the field sleep.
sleepTag() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Causes a tag in the field to enter the sleep state.
startService() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Starts up this `NetworkDiscoveryListenerService`.
startService(boolean) - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Starts up this `NetworkDiscoveryListenerService`.
startService() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Starts up this `SerialDiscoveryListenerService`.
startService() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Starts this `MessageListenerService`.
status - Variable in class com.alien.enterpriseRFID.reader.AlienDLEObject
stopService() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Stops this `NetworkDiscoveryListenerService`.
stopService() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Stops this `SerialDiscoveryListenerService`.
stopService() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Stops this `MessageListenerService`.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X