Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

# Constant Field Values

Contents

- com.alien.*

com.alien.*

com.alien.enterpriseRFID.discovery.DiscoveryItem
`public static final java.lang.String` | `AUTOMATIC` | `"Automatic"`
`public static final java.lang.String` | `MANUAL` | `"Manual"`
`public static final java.lang.String` | `NETWORK` | `"Network"`
`public static final java.lang.String` | `SERIAL` | `"Serial"`

com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
`public static final int` | `DEFAULT_LISTENER_PORT` | `3988`
`public static final int` | `DEFAULT_LISTENER_TIMEOUT_SECONDS` | `2`

com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
`public static final int` | `SCANNING_END` | `2`
`public static final int` | `SCANNING_PORT` | `1`
`public static final int` | `SCANNING_PORTBUSY` | `3`

com.alien.enterpriseRFID.externalio.ExternalIO
`public static final int` | `DI` | `1`
`public static final int` | `DO` | `2`

com.alien.enterpriseRFID.notify.Message
`public static final java.lang.String` | `REASON_IOSTREAM` | `"IO STREAM"`
`public static final java.lang.String` | `REASON_TAGSTREAM` | `"TAG STREAM"`

com.alien.enterpriseRFID.reader.AbstractReader
`public static final int` | `DEBUG_BYTES` | `2`
`public static final int` | `DEBUG_OFF` | `0`
`public static final int` | `DEBUG_TEXT` | `1`
`public static final int` | `DEFAULT_TIMEOUT` | `10000`
`public static final int` | `TIMEOUTMODE_CHARACTER` | `1`
`public static final int` | `TIMEOUTMODE_COMMAND` | `0`

com.alien.enterpriseRFID.reader.AlienClass1Reader
`public static final java.lang.String` | `ALL_MASK` | `"All"`
`public static final int` | `CLASS0` | `8`
`public static final int` | `CLASS1GEN1_64BITS` | `3`
`public static final int` | `CLASS1GEN1_96BITS` | `4`
`public static final int` | `CLASS1GEN1_ALL` | `7`
`public static final int` | `CLASS1GEN1_LEPTON` | `4`
`public static final int` | `CLASS1GEN1_OMEGA` | `2`
`public static final int` | `CLASS1GEN1_QUARK` | `1`
`public static final int` | `CLASS1GEN2` | `16`
`public static final java.lang.String` | `CUSTOM_FORMAT` | `"Custom"`
`public static final java.lang.String` | `DATA_INC_ALWAYS` | `"Always"`
`public static final java.lang.String` | `DATA_INC_FAIL` | `"Fail"`
`public static final java.lang.String` | `DATA_INC_OFF` | `"OFF"`
`public static final java.lang.String` | `DATA_INC_SUCCESS` | `"Success"`
`public static final java.lang.String` | `DATA_INC_WRITE` | `"Write"`
`public static final java.lang.String` | `FUNCTION_PROGRAMMER` | `"Programmer"`
`public static final java.lang.String` | `FUNCTION_READER` | `"Reader"`
`public static final java.lang.String` | `G2TARGET_A` | `"A"`
`public static final java.lang.String` | `G2TARGET_AB` | `"AB"`
`public static final java.lang.String` | `G2TARGET_B` | `"B"`
`public static final java.lang.String` | `GLOBAL_SCROLL` | `"Global Scroll"`
`public static final java.lang.String` | `INVENTORY` | `"Inventory"`
`public static final java.lang.String` | `LOCKTYPE_LOCK` | `"Lock"`
`public static final java.lang.String` | `LOCKTYPE_PERMALOCK` | `"PermaLock"`
`public static final java.lang.String` | `LOCKTYPE_PERMAUNLOCK` | `"PermaUnlock"`
`public static final int` | `LOG_OFF` | `0`
`public static final int` | `LOG_ON` | `1`
`public static final int` | `OFF` | `0`
`public static final int` | `ON` | `1`
`public static final int` | `PROG_CLASS0` | `0`
`public static final int` | `PROG_CLASS1GEN1` | `1`
`public static final int` | `PROG_CLASS1GEN2` | `2`
`public static final java.lang.String` | `RFMOD_DRM` | `"DRM"`
`public static final java.lang.String` | `RFMOD_HS` | `"HS"`
`public static final java.lang.String` | `RFMOD_STD` | `"STD"`
`public static final java.lang.String` | `TERSE_FORMAT` | `"Terse"`
`public static final java.lang.String` | `TEXT_FORMAT` | `"Text"`
`public static final java.lang.String` | `XML_FORMAT` | `"XML"`

com.alien.enterpriseRFID.reader.AlienClassBPTReader
`public static final int` | `DEFAULT_TIMEOUT` | `20000`
`public static final short` | `NO_READING` | `9999`
`public static final short` | `NO_WRITING` | `9999`

com.alien.enterpriseRFID.reader.AlienDLEObject
`public static final int` | `CMD_DIRECTED_INV_LIST_CONTROL` | `66`
`public static final int` | `CMD_ENTER_BOOTLOADER` | `209`
`public static final int` | `CMD_ERASE_TAG` | `81`
`public static final int` | `CMD_FORMAT_TAG_MEMORY` | `39`
`public static final int` | `CMD_GET_ACTIVE_ANTENNA` | `8`
`public static final int` | `CMD_GET_ANTENNA_RF_POWER` | `98`
`public static final int` | `CMD_GET_ANTENNA_SEQUENCE` | `29`
`public static final int` | `CMD_GET_BIDIRECTIONAL_DDR` | `23`
`public static final int` | `CMD_GET_FIRMWARE_VERSION` | `0`
`public static final int` | `CMD_GET_HARDWARE_INFO` | `17`
`public static final int` | `CMD_GET_IO_INVERSION_MASK` | `12`
`public static final int` | `CMD_GET_IO_PORT_VALUE` | `6`
`public static final int` | `CMD_GET_IO_STATUS_LATCH` | `25`
`public static final int` | `CMD_GET_LOGGING` | `41`
`public static final int` | `CMD_GET_LOGGING_INTERVAL` | `43`
`public static final int` | `CMD_GET_MANUFACTURING_INFO` | `18`
`public static final int` | `CMD_GET_OUTPUT_INITIAL_STATE` | `31`
`public static final int` | `CMD_GET_READER_NUMBER` | `2`
`public static final int` | `CMD_GET_READER_STATUS` | `15`
`public static final int` | `CMD_GET_RF_ATTENUATION` | `10`
`public static final int` | `CMD_GET_RF_ONOFF` | `27`
`public static final int` | `CMD_GET_SENSOR_IMMEDIATE` | `50`
`public static final int` | `CMD_GET_TAG_FIRMWARE_VERSION` | `32`
`public static final int` | `CMD_GET_TAG_ID` | `36`
`public static final int` | `CMD_GET_TAG_MASK` | `21`
`public static final int` | `CMD_GET_TAG_MEMORY` | `38`
`public static final int` | `CMD_GET_TAG_MODE` | `49`
`public static final int` | `CMD_GET_TAG_TYPE` | `47`
`public static final int` | `CMD_GET_TIME` | `45`
`public static final int` | `CMD_GLOBALSCROLL_TAG` | `62`
`public static final int` | `CMD_INTERNAL_TEST_PROCEDURE` | `13`
`public static final int` | `CMD_INV_DIAGNOSTIC_CONTROL` | `78`
`public static final int` | `CMD_INVENTORY` | `64`
`public static final int` | `CMD_KILL_TAG` | `82`
`public static final int` | `CMD_LOCK_TAG` | `83`
`public static final int` | `CMD_MANAGE_RESERVED_PARAMS` | `19`
`public static final int` | `CMD_PROGRAM_ROW` | `35`
`public static final int` | `CMD_PROGRAM_TAG` | `80`
`public static final int` | `CMD_READ_TAG_DATA` | `255`
`public static final int` | `CMD_REBOOT` | `4`
`public static final int` | `CMD_RESTORE_FACTORY_DEFAULTS` | `16`
`public static final int` | `CMD_SET_ACTIVE_ANTENNA` | `7`
`public static final int` | `CMD_SET_ANTENNA_RF_POWER` | `97`
`public static final int` | `CMD_SET_ANTENNA_SEQUENCE` | `28`
`public static final int` | `CMD_SET_BAUD_RATE` | `3`
`public static final int` | `CMD_SET_BIDIRECTIONAL_DDR` | `22`
`public static final int` | `CMD_SET_IO_INVERSION_MASK` | `11`
`public static final int` | `CMD_SET_IO_MASK` | `24`
`public static final int` | `CMD_SET_IO_PORT_VALUE` | `5`
`public static final int` | `CMD_SET_LOGGING` | `40`
`public static final int` | `CMD_SET_LOGGING_INTERVAL` | `42`
`public static final int` | `CMD_SET_OUTPUT_INITIAL_STATE` | `30`
`public static final int` | `CMD_SET_READER_NUMBER` | `1`
`public static final int` | `CMD_SET_RF_ATTENUATION` | `9`
`public static final int` | `CMD_SET_RF_ONOFF` | `26`
`public static final int` | `CMD_SET_TAG_MASK` | `20`
`public static final int` | `CMD_SET_TAG_MEMORY` | `37`
`public static final int` | `CMD_SET_TAG_MODE` | `48`
`public static final int` | `CMD_SET_TAG_TYPE` | `46`
`public static final int` | `CMD_SET_TIME` | `44`
`public static final int` | `CMD_SLEEP_TAG` | `33`
`public static final int` | `CMD_SUSPEND_READER` | `14`
`public static final int` | `CMD_UPLOAD_FIRMWARE_LINE` | `210`
`public static final int` | `CMD_VERIFY_TAG` | `61`
`public static final int` | `CMD_WAKE_N` | `65`
`public static final int` | `CMD_WAKE_TAG` | `34`
`public static final int` | `COMMAND_BUFFER_SIZE` | `100`
`public static final int` | `COMMAND_DLE` | `16`
`public static final int` | `COMMAND_EOF` | `2`
`public static final int` | `COMMAND_SOF` | `1`
`public static final int` | `COMMAND_STATUS_COMPLETE` | `10`
`public static final int` | `COMMAND_STATUS_ERROR` | `11`
`public static final int` | `COMMAND_STATUS_INVENTORY_BREAK` | `5`
`public static final int` | `COMMAND_STATUS_READER_ERROR` | `20`
`public static final int` | `COMMAND_STATUS_RECEIVE_ME` | `3`
`public static final int` | `COMMAND_STATUS_RESET` | `1`
`public static final int` | `COMMAND_STATUS_SEND_ME` | `2`
`public static final int` | `COMMAND_STATUS_TIMEOUT` | `12`
`public static final int` | `COMMAND_STATUS_UNKNOWN` | `0`
`public static final int` | `REPLY_BUFFER_SIZE` | `100`
`public static final int` | `RESPONSE_DATA_SIZE_MISMATCH` | `140`
`public static final int` | `RESPONSE_DIAGNOSTIC_DATA` | `8`
`public static final int` | `RESPONSE_DIAGNOSTIC_END` | `9`
`public static final int` | `RESPONSE_DIAGNOSTIC_START` | `7`
`public static final int` | `RESPONSE_ERASE_FAILED` | `135`
`public static final int` | `RESPONSE_HARDWARE_ERROR` | `141`
`public static final int` | `RESPONSE_INVALID_KILL_CODE` | `148`
`public static final int` | `RESPONSE_INVENTORY_END` | `3`
`public static final int` | `RESPONSE_INVENTORY_START` | `1`
`public static final int` | `RESPONSE_INVENTORY_TAG` | `2`
`public static final int` | `RESPONSE_KILL_FAILED` | `138`
`public static final int` | `RESPONSE_LIST_DUMP_END` | `6`
`public static final int` | `RESPONSE_LIST_DUMP_RECORD` | `5`
`public static final int` | `RESPONSE_LIST_DUMP_START` | `4`
`public static final int` | `RESPONSE_LIST_FULL` | `142`
`public static final int` | `RESPONSE_LOCK_CRC_ERROR` | `146`
`public static final int` | `RESPONSE_LOCK_FAILED` | `139`
`public static final int` | `RESPONSE_MESSAGE_OK` | `0`
`public static final int` | `RESPONSE_MESSAGE_OK_G2` | `16`
`public static final int` | `RESPONSE_NO_TAG` | `134`
`public static final int` | `RESPONSE_OVERFLOW_ERROR` | `133`
`public static final int` | `RESPONSE_PROGRAM_FAILED` | `136`
`public static final int` | `RESPONSE_RESUME` | `13`
`public static final int` | `RESPONSE_SUSPEND` | `12`
`public static final int` | `RESPONSE_TAG_LOCKED` | `137`
`public static final int` | `RESPONSE_TAG_LOST` | `147`
`public static final int` | `RESPONSE_UNKNOWN_COMMAND` | `131`
`public static final int` | `RESPONSE_UNKNOWN_LENGTH` | `129`
`public static final int` | `RESPONSE_UNKNOWN_TAG_COMMAND` | `132`
`public static final int` | `RESPONSE_UNKNOWN_VALUE` | `130`
`public static final int` | `RESPONSE_UPLOAD_CRC_ERROR` | `145`
`public static final int` | `RESPONSE_UPLOAD_END` | `11`
`public static final int` | `RESPONSE_UPLOAD_INVALID` | `144`
`public static final int` | `RESPONSE_UPLOAD_LINE_ERROR` | `143`
`public static final int` | `RESPONSE_UPLOAD_OK` | `10`
`public static final int` | `SUBCMD_AVAILABLE_BAUD_RATES` | `16`
`public static final int` | `SUBCMD_BIDIRECTIONAL_IO` | `3`
`public static final int` | `SUBCMD_GENERAL_PURPOSE_INPUTS` | `2`
`public static final int` | `SUBCMD_GENERAL_PURPOSE_OUTPUTS` | `1`
`public static final int` | `SUBCMD_GET_AIR_INTERFACE_BAUD` | `138`
`public static final int` | `SUBCMD_GET_CAL_TABLE_ENTRY` | `140`
`public static final int` | `SUBCMD_GET_DECODE_PARAMETERS` | `171`
`public static final int` | `SUBCMD_GET_DIAGNOSTIC_MODE` | `162`
`public static final int` | `SUBCMD_GET_ETSI_LISTEN_PARAMS` | `183`
`public static final int` | `SUBCMD_GET_HOP_TABLE_ENTRY` | `146`
`public static final int` | `SUBCMD_GET_MOD_CONTROL_MANUAL` | `130`
`public static final int` | `SUBCMD_GET_MOD_FUDGE` | `177`
`public static final int` | `SUBCMD_GET_NV_RAW` | `142`
`public static final int` | `SUBCMD_GET_PA_BIAS` | `132`
`public static final int` | `SUBCMD_GET_PA_VDD` | `134`
`public static final int` | `SUBCMD_GET_PING_PARAMS` | `181`
`public static final int` | `SUBCMD_GET_PROGRAM_LENGTH` | `167`
`public static final int` | `SUBCMD_GET_PROGRAM_POWER_LEVELS` | `169`
`public static final int` | `SUBCMD_GET_RAW_MEMORY` | `165`
`public static final int` | `SUBCMD_GET_RAW_RF_POWER` | `150`
`public static final int` | `SUBCMD_GET_RECEIVER_GAIN` | `136`
`public static final int` | `SUBCMD_GET_SUSPENDERS_PARAMS` | `179`
`public static final int` | `SUBCMD_GET_TREE_INV_METHOD` | `174`
`public static final int` | `SUBCMD_HOP_INTERVAL` | `19`
`public static final int` | `SUBCMD_HOP_STEP_SIZE` | `10`
`public static final int` | `SUBCMD_LOCALIZATION` | `6`
`public static final int` | `SUBCMD_MAX_DIRECTED_SORT_LIST` | `17`
`public static final int` | `SUBCMD_MAXIMUM_ANTENNA_NUMBER` | `22`
`public static final int` | `SUBCMD_MAXIMUM_FREQUENCY` | `9`
`public static final int` | `SUBCMD_MAXIMUM_HOP_TABLE_INDEX` | `4`
`public static final int` | `SUBCMD_MAXIMUM_RF_CHANNEL` | `12`
`public static final int` | `SUBCMD_MAXIMUM_RF_POWER` | `13`
`public static final int` | `SUBCMD_MINIMUM_FREQUENCY` | `8`
`public static final int` | `SUBCMD_OPERATING_VOLTAGE` | `14`
`public static final int` | `SUBCMD_PLL_TYPE` | `11`
`public static final int` | `SUBCMD_PROGRAMMER_ENABLE` | `0`
`public static final int` | `SUBCMD_RADIO_TYPE` | `7`
`public static final int` | `SUBCMD_READER_TYPE` | `5`
`public static final int` | `SUBCMD_RESTORE_DEFAULT_HOP` | `144`
`public static final int` | `SUBCMD_RESTORE_DEFAULT_NV` | `143`
`public static final int` | `SUBCMD_RF_CHANNEL` | `21`
`public static final int` | `SUBCMD_SEND_MODULATION_CONT` | `128`
`public static final int` | `SUBCMD_SEND_PRIMITIVE_ONE_SHOT` | `163`
`public static final int` | `SUBCMD_SET_AIR_INTERFACE_BAUD` | `137`
`public static final int` | `SUBCMD_SET_CAL_TABLE_ENTRY` | `139`
`public static final int` | `SUBCMD_SET_DECODE_DIAG` | `172`
`public static final int` | `SUBCMD_SET_DECODE_PARAMETERS` | `170`
`public static final int` | `SUBCMD_SET_DIAGNOSTIC_MODE` | `161`
`public static final int` | `SUBCMD_SET_ETSI_LISTEN_CHANNEL` | `175`
`public static final int` | `SUBCMD_SET_ETSI_LISTEN_PARAMS` | `182`
`public static final int` | `SUBCMD_SET_HOP_TABLE_ENTRY` | `145`
`public static final int` | `SUBCMD_SET_MOD_CONTROL_MANUAL` | `129`
`public static final int` | `SUBCMD_SET_MOD_FUDGE` | `176`
`public static final int` | `SUBCMD_SET_NV_RAW` | `141`
`public static final int` | `SUBCMD_SET_PA_BIAS` | `131`
`public static final int` | `SUBCMD_SET_PA_VDD` | `133`
`public static final int` | `SUBCMD_SET_PING_PARAMS` | `180`
`public static final int` | `SUBCMD_SET_PROGRAM_LENGTH` | `166`
`public static final int` | `SUBCMD_SET_PROGRAM_POWER_LEVELS` | `168`
`public static final int` | `SUBCMD_SET_RADIO_MANUF_INFO` | `148`
`public static final int` | `SUBCMD_SET_RAW_MEMORY` | `164`
`public static final int` | `SUBCMD_SET_RAW_RF_POWER` | `149`
`public static final int` | `SUBCMD_SET_READER_MANUF_INFO` | `147`
`public static final int` | `SUBCMD_SET_RECEIVER_GAIN` | `135`
`public static final int` | `SUBCMD_SET_SUSPENDERS_PARAMS` | `178`
`public static final int` | `SUBCMD_SET_TREE_INV_METHOD` | `173`
`public static final int` | `SUBCMD_SUPPORTED_TAG_TYPES` | `18`
`public static final int` | `SUBCMD_VOLTAGE_CALIBRATION` | `151`
`public static final int` | `TAGDECODE_COLLISION` | `2`
`public static final int` | `TAGDECODE_CRC_ERROR` | `3`
`public static final int` | `TAGDECODE_GOOD_ID` | `0`
`public static final int` | `TAGDECODE_NO_TAG` | `1`
`public static final int` | `WAITING_FOR_DLE` | `0`
`public static final int` | `WAITING_FOR_DLE_EMBEDDED` | `3`
`public static final int` | `WAITING_FOR_MSG` | `2`
`public static final int` | `WAITING_FOR_SOF` | `1`

com.alien.enterpriseRFID.tags.Tag
`public static final int` | `DIR_AWAY` | `1`
`public static final int` | `DIR_STATIC` | `0`
`public static final int` | `DIR_TOWARD` | `-1`
`public static final int` | `FOREVER` | `-1`
`public static final int` | `PROTO_C0` | `0`
`public static final int` | `PROTO_C1G1` | `1`
`public static final int` | `PROTO_C1G2` | `2`
`public static final int` | `PROTO_UNKNOWN` | `-1`

com.alien.enterpriseRFID.tags.TagTable
`public static final int` | `FOREVER` | `-1`

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES