# Package com.atid.lib.module.barcode.ssi.type

- Class Summary
  Class | Description
  --- | ---
  CodeLength | The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.

- Enum Summary
  Enum | Description
  --- | ---
  AustraliaPostFormat | To select one of the following formats for Australia Post,
  AztecInverse | This parameter sets the Aztec inverse decoder setting.
  BooklandISBNFormat | If Bookland EAN is enabled, select one of the following formats for Bookland data - Bookland ISBN-10 / Bookland ISBN-13
  CodabarStartStopCharactersDetection | Select whether to detect upper case or lower case Codabar start/stop characters.
  Code11CheckDigitVerification | This feature allows the decoder to check the integrity of all Code 11 symbols to verify that the data complies with the specified check digit algorithm.
  CodeLengthType | The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
  CompositeBeepMode | To select the number of decode beeps when a composite bar code is decoded, scan the appropriate bar code.
  CouponReport | Traditional coupon symbols (old coupon symbols) are composed of two bar codes: UPC/EAN and Code128.
  DataMatrixInverse | This parameter sets the Data Matrix inverse decoder setting.
  DecodeMirrorImages | Select an option for decoding mirror image Data Matrix bar codes (Data Matrix Only)
  DecodeUpcEanJanSupplementals | Supplementals are bar codes appended according to specific format conventions (e.g., UPC A+2, UPC E+2, EAN 13+2).
  GS1DataBarLimitedSecurityLevel | The decoder offers four levels of decode security for GS1 DataBar Limited bar codes.
  HanXinInverse | This parameter sets the 1D inverse decoder setting.
  I2of5CheckDigitVerification | Enable this feature to check the integrity of all I 2 of 5 symbols to verify the data complies with either the specified Uniform Symbology Specification (USS), or the Optical Product Code Council (OPCC) check digit algorithm.
  I2of5SecurityLevel | Interleaved 2 of 5 bar codes are vulnerable to misdecodes by the nature of the symbol, especially when Any Length is set for Interleaved 2 of 5 bar codes.
  IntercharacterGapSize | The Code 39 and Codabar symbologies have an intercharacter gap that is typically quite small.
  Inverse1D | This parameter sets the 1D inverse decoder setting.
  ISBTConcatenation | Select an option for concatenating pairs of ISBT code types
  LinearSecurityLevel | The 1D Barcode Scanner offers four levels of decode security for linear code types (e.g.
  MSICheckDigitAlgorithm | Two algorithms are possible for the verification of the second MSI check digit.
  MSICheckDigits | With MSI symbols, one check digit is mandatory and always verified by the reader.
  Preamble | Preamble characters are part of the UPC symbol, and include Country Code and System Character.
  QRInverse | This parameter sets the QR inverse decoder setting.
  QuietZoneLevel1D | This feature sets the level of aggressiveness in decoding bar codes with a reduced quiet zone (the area in front of and at the end of a bar code), and applies to symbologies enabled by a Reduced Quiet Zone parameter.
  RedundancyLevel | The decoder offers four levels of decode redundancy.
  SecurityLevel | The decoder offers four levels of decode security for delta bar codes, which include UPC/EAN and Code 93.
  UpcCompositeMode | If you enable Composite CC-A/B , select an option for linking UPC symbols with a 2D symbol during transmission as if they were one symbol
  UpcEanJanSupplementalAIMIDFormat | Select an output format when reporting UPC/EAN/JAN bar codes with Supplementals with Transmit Code ID Character set to AIM Code ID Character:
  UpcEanSecurityLevel | The 1D Barcode Scanner offers four levels of decode security for UPC/EAN bar codes.