A B C D E F G H I K L M N O P Q R S T U V W

## W

wakeUp() - Method in class com.atid.lib.atx88.ATx88Reader
wakeUp(IATEAReaderEventListener) - Method in class com.atid.lib.atx88.ATx88Reader
wakeUp() - Method in class com.atid.lib.reader.ATEAReader
  An instance of the ATEAReader class is called when an active Host device is in the Sleep state and wakes up.
wakeUp(IATEAReaderEventListener) - Method in class com.atid.lib.reader.ATEAReader
  An instance of the ATEAReader class is called when an active Host device is in the Sleep state and wakes up.
write(byte[]) - Method in class com.atid.lib.transport.ATransport
  Transfer data to the device.
write(byte[], int) - Method in class com.atid.lib.transport.ATransport
  Transfer data to the device.
write(byte[], int, int) - Method in class com.atid.lib.transport.ATransport
  Transfer data to the device.
write(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransport
  Transfer data to the device.
write(byte[], int, int) - Method in class com.atid.lib.transport.ATransportBluetooth
write(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportBluetooth
write(byte[], int, int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
write(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
write(byte[], int, int) - Method in class com.atid.lib.transport.ATransportUsb
write(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportUsb
writememory6b(int, String, String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
writememory6b(int, String, String) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to store data in a specific memory of RFID UHF tag of ISO18000-6b Gen2 standard.
writeMemory6c(BankType, int, String, String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
writeMemory6c(BankType, int, String, String) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to store data in a specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.

A B C D E F G H I K L M N O P Q R S T U V W