A B C D E F G H I K L M N O P Q R S T U V W

## M

mAction - Variable in class com.atid.lib.reader.ATEAReader
mAddress - Variable in class com.atid.lib.transport.ATransport
Mask6cAction - Enum in com.atid.lib.module.rfid.uhf.types
  The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
Mask6cPattern - Class in com.atid.lib.module.rfid.uhf.params
  The Mask6cPattern class is a class that represents the Mask Pattern of a Selection Mask in terms of pattern and length.
Mask6cPattern() - Constructor for class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(<any>) - Constructor for class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cPattern(String, int) - Constructor for class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Create an instance of the Mask6cPattern class.
Mask6cTarget - Enum in com.atid.lib.module.rfid.uhf.types
  The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
MAX_METHOD - Static variable in class com.atid.lib.reader.params.NotifyMethod
MAX_PARAM - Static variable in class com.atid.lib.module.barcode.ATBarcode
mBarcode - Variable in class com.atid.lib.reader.ATEAReader
mBarcodeNames - Variable in class com.atid.lib.module.barcode.ATBarcode
mCheckBatteryInterval - Variable in class com.atid.lib.reader.ATEAReader
mConnType - Variable in class com.atid.lib.transport.ATransport
mDefaultOption - Variable in class com.atid.lib.module.barcode.ATBarcode
mDefaultState - Variable in class com.atid.lib.module.barcode.ATBarcode
mDevice - Variable in class com.atid.lib.reader.ATEAReader
mDeviceVersion - Variable in class com.atid.lib.reader.ATEAReader
mDevName - Variable in class com.atid.lib.transport.ATransport
mDevType - Variable in class com.atid.lib.transport.ATransport
mFailCount - Variable in class com.atid.lib.reader.ATEAReader
mIsAutoConnect - Variable in class com.atid.lib.transport.ATransport
mIsDeviceAttached - Variable in class com.atid.lib.transport.ATransport
mIsDisconnecting - Variable in class com.atid.lib.reader.ATEAReader
mIsForceBatteryGauging - Variable in class com.atid.lib.reader.ATEAReader
mLastError - Variable in class com.atid.lib.reader.ATEAReader
mLastTime - Variable in class com.atid.lib.reader.ATEAReader
mListeners - Variable in class com.atid.lib.module.barcode.ATBarcode
mListeners - Variable in class com.atid.lib.module.rfid.uhf.ATRfidUhf
mMacAddress - Variable in class com.atid.lib.transport.ATransport
mModule - Variable in class com.atid.lib.module.barcode.ATBarcode
mModule - Variable in class com.atid.lib.module.rfid.uhf.ATRfidUhf
ModuleBarcodeProtocolType - Enum in com.atid.lib.types
ModuleBarcodeType - Enum in com.atid.lib.types
  The ModuleBarcodeType enumeration indicates the type of Barcode Module installed in the instrument.
ModuleRfidHfType - Enum in com.atid.lib.types
  The ModuleRfidHfType enumeration indicates the type of RFID HF Module installed in the instrument.
ModuleRfidUhfType - Enum in com.atid.lib.types
  The ModuleRfidUhfType enumeration indicates the type of RFID UHF Module installed in the instrument.
mQueue - Variable in class com.atid.lib.transport.ATransport
mReader - Variable in class com.atid.lib.module.barcode.ATBarcode
mReader - Variable in class com.atid.lib.module.rfid.uhf.ATRfidUhf
mRfidHf - Variable in class com.atid.lib.reader.ATEAReader
mRfidUhf - Variable in class com.atid.lib.reader.ATEAReader
MSICheckCharacter - Enum in com.atid.lib.module.barcode.spc.type
  Different types of check characters are used with MSI bar codes.
MSICheckDigitAlgorithm - Enum in com.atid.lib.module.barcode.ssi.type
  Two algorithms are possible for the verification of the second MSI check digit.
MSICheckDigits - Enum in com.atid.lib.module.barcode.ssi.type
  With MSI symbols, one check digit is mandatory and always verified by the reader.
mState - Variable in class com.atid.lib.transport.ATransport
mTransport - Variable in class com.atid.lib.reader.ATEAReader

A B C D E F G H I K L M N O P Q R S T U V W