A B C D E F G H I K L M N O P Q R S T U V W

## R

read(byte[]) - Method in class com.atid.lib.transport.ATransport
  Read data received from the device.
read(byte[], int) - Method in class com.atid.lib.transport.ATransport
  Read data received from the device.
read(byte[], int, int) - Method in class com.atid.lib.transport.ATransport
  Read data received from the device.
read(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransport
  Read data received from the device.
read(byte[], int, int) - Method in class com.atid.lib.transport.ATransportBluetooth
read(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportBluetooth
read(byte[], int, int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
read(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
read(byte[], int, int) - Method in class com.atid.lib.transport.ATransportUsb
read(byte[], int, int, int) - Method in class com.atid.lib.transport.ATransportUsb
readMemory6b(int, int, String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
readMemory6b(int, int, String) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to read specific memory of RFID UHF tag of ISO18000-6b Gen2 standard.
readMemory6c(BankType, int, int, String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
readMemory6c(BankType, int, int, String) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to read specific memory of RFID UHF tag of ISO18000-6c Gen2 standard.
RedundancyLevel - Enum in com.atid.lib.module.barcode.ssi.type
  The decoder offers four levels of decode redundancy.
removeAllStoreadData() - Method in class com.atid.lib.atx88.ATx88Reader
removeAllStoreadData() - Method in class com.atid.lib.reader.ATEAReader
  Deletes all data stored in the device.
removeListener(IATBarcodeEventListener) - Method in class com.atid.lib.module.barcode.ATBarcode
  Removes an event handler when it no longer needs to receive events from the ATBarcode instance.
removeListener(IATRfidUhfEventListener) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  ATRfidUhf Removes an event handler when it no longer needs to receive events raised by the instance.
removeListener(IATEAReaderEventListener) - Method in class com.atid.lib.reader.ATEAReader
  Removes the Listener that is listening for events on an instance of the ATEAReader class.
reset() - Method in class com.atid.lib.atx88.ATx88Reader
reset() - Method in class com.atid.lib.reader.ATEAReader
  Reset the device.
resetError() - Method in class com.atid.lib.reader.ATEAReader
ResponseType - Enum in com.atid.lib.module.barcode.spc.type
  The device responds to serial commands with one of three responses: ACK (0x06) Indicates a good command which has been processed.
ResultCode - Enum in com.atid.lib.types
  The ResultCode enumeration represents failure and behavior results.
RETRY_COUNT - Static variable in class com.atid.lib.reader.ATEAReader

A B C D E F G H I K L M N O P Q R S T U V W