A B C D E F G H I K L M N O P Q R S T U V W

## A

ActionState - Enum in com.atid.lib.types
  ActionState indicates the current operation status of the device.
ActionType - Enum in com.atid.lib.types
add(BarcodeType, boolean) - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Add symbol state information to the SymbolStateList instance.
add(SPCParamName) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Add parameter type to the SPCParamNameList instance.
add(SPCParamName[]) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Add all the information for the SPCParamNameList instance.
add(SPCParamValue) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Add parameter information to the SPCParamValueList instance.
add(SPCParamValue[]) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Add all the information for the SPCParamValueList instance.
add(SSI1DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Add parameter type to the SSI1DParamNameList instance.
add(SSI1DParamName[]) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Add all the information for the SSI1DParamNameList instance.
add(SSI1DParamValue) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Add parameter information to the SSI1DParamValueList instance.
add(SSI1DParamValue[]) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Add all the information for the SSI1DParamValueList instance.
add(SSI1DParamName, Object) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Add parameter information to the SSI1DParamValueList instance.
add(SSI2DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Add parameter type to the SSI2DParamNameList instance.
add(SSI2DParamName[]) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Add all the information for the SSI2DParamNameList instance.
add(SSI2DParamValue) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Add parameter information to the SSI2DParamValueList instance.
add(SSI2DParamValue[]) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Add all the information for the SSI2DParamValueList instance.
add(SSI2DParamName, Object) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Add parameter information to the SSI2DParamValueList instance.
addAll(SymbolStateList) - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Add all the information for the SymbolStateList instance.
addEpcMask(EpcMaskParam) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
addEpcMask(EpcMaskParam) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Add the EPC Mask of the RFID UHF module of the Device.
addListener(IATBarcodeEventListener) - Method in class com.atid.lib.module.barcode.ATBarcode
  Add an event handler to receive events from the ATBarcode instance.
addListener(IATRfidUhfEventListener) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  ATRfidUhf Adds an event handler to receive events that occur in the instance.
addListener(IATEAReaderEventListener) - Method in class com.atid.lib.reader.ATEAReader
  Adds a Listener to receive events on an instance of the ATEAReader class.
AlgorithmType - Enum in com.atid.lib.module.rfid.uhf.types
  The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
assertAction() - Method in class com.atid.lib.atx88.ATx88Reader
assertAction() - Method in class com.atid.lib.module.barcode.ATBarcode
assertAction(byte[]) - Method in class com.atid.lib.module.barcode.ATBarcode
assertAction() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
assertModule() - Method in class com.atid.lib.module.barcode.ATBarcode
assertModule(byte[]) - Method in class com.atid.lib.module.barcode.ATBarcode
assertModule() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
AT188Reader - Class in com.atid.lib.atx88
  The AT188Reader class implements the unique capabilities of the AT188N Device.
AT188Reader(ATransport) - Constructor for class com.atid.lib.atx88.AT188Reader
  Create an instance of the AT188Reader class.
AT188Reader(int, ATransport) - Constructor for class com.atid.lib.atx88.AT188Reader
  Create an instance of the AT188Reader class.
AT388Reader - Class in com.atid.lib.atx88
  The AT388Reader class implements the unique capabilities of the AT388 Device.
AT388Reader(ATransport) - Constructor for class com.atid.lib.atx88.AT388Reader
  Create an instance of the AT388Reader class.
AT388Reader(int, ATransport) - Constructor for class com.atid.lib.atx88.AT388Reader
  Create an instance of the AT388Reader class.
ATBarcode - Class in com.atid.lib.module.barcode
  The ATBarcode class provides the ability to control the Barcode module installed on the Device when the ATEAReader instance is connected to the Device.
ATBarcode(IReader) - Constructor for class com.atid.lib.module.barcode.ATBarcode
  Create an instance of the ATBarcode class.
ATEAReader - Class in com.atid.lib.reader
  The ATEAReader class is a class that controls EAD in connection with ATID's EAD equipment, receives data from EAD, and delivers it to the application program.
ATEAReader(ATransport) - Constructor for class com.atid.lib.reader.ATEAReader
  Creates an instance of ATEAReader.
ATEAReader(int, ATransport) - Constructor for class com.atid.lib.reader.ATEAReader
  Creates an instance of ATEAReader.
ATException - Exception in com.atid.lib.diagnostics
ATException(ResultCode) - Constructor for exception com.atid.lib.diagnostics.ATException
  Constructs an instance of ATException.
ATn88Reader - Class in com.atid.lib.atx88
  The ATn88Reader class implements the common functions of AT188N Device and AT388 Device.
ATn88Reader(ATransport) - Constructor for class com.atid.lib.atx88.ATn88Reader
  Create an instance of the ATn88Reader class.
ATn88Reader(int, ATransport) - Constructor for class com.atid.lib.atx88.ATn88Reader
  Create an instance of the ATn88Reader class.
ATransport - Class in com.atid.lib.transport
  The Transport class is a class for abstracting connections with Reader devices.
ATransport() - Constructor for class com.atid.lib.transport.ATransport
  Create an instance of the Transport class
ATransport(DeviceType, String, String) - Constructor for class com.atid.lib.transport.ATransport
  Create an instance of the Transport class
ATransport(DeviceType, String, String, boolean) - Constructor for class com.atid.lib.transport.ATransport
  Create an instance of the Transport class
ATransport(DeviceType, String, String, String) - Constructor for class com.atid.lib.transport.ATransport
  Create an instance of the Transport class
ATransport(DeviceType, String, String, String, boolean) - Constructor for class com.atid.lib.transport.ATransport
  Create an instance of the Transport class
ATransport.IBufferControlEventListener - Interface in com.atid.lib.transport
  The interface for software flow control according to the state of the Transport internal buffer while the Transport instance is communicating with the device.
ATransport.IConnectStateEventListener - Interface in com.atid.lib.transport
  It is an interface to notify the connection status with the equipment.
ATransportBluetooth - Class in com.atid.lib.transport
  The Transport class is a class for abstracting connections with Reader devices.
ATransportBluetooth() - Constructor for class com.atid.lib.transport.ATransportBluetooth
  Create an instance of the ATransportBluetooth class
ATransportBluetooth(DeviceType, String, String) - Constructor for class com.atid.lib.transport.ATransportBluetooth
  Create an instance of the ATransportBluetooth class
ATransportBluetoothLe - Class in com.atid.lib.transport
ATransportBluetoothLe() - Constructor for class com.atid.lib.transport.ATransportBluetoothLe
  Create an instance of the ATransportBluetooth class
ATransportBluetoothLe(DeviceType, String, String) - Constructor for class com.atid.lib.transport.ATransportBluetoothLe
  Create an instance of the ATransportBluetooth class
ATransportUsb - Class in com.atid.lib.transport
ATransportUsb() - Constructor for class com.atid.lib.transport.ATransportUsb
  Create an instance of the ATransportUsb class
ATransportUsb(DeviceType, String, String) - Constructor for class com.atid.lib.transport.ATransportUsb
  Create an instance of the ATransportUsb class
ATransportUsb(DeviceType, String, String, boolean) - Constructor for class com.atid.lib.transport.ATransportUsb
  Create an instance of the ATransportUsb class
ATRfidUhf - Class in com.atid.lib.module.rfid.uhf
  ATRfidUhf class is a class that provides the function to control RFID UHF module installed in Device when ATEAReader instance is connected to Device.
ATRfidUhf(IReader) - Constructor for class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Create an instance of the ATRfidUhf class.
ATRfidUhfATM - Class in com.atid.lib.module.rfid.uhf.atm
  The ATRfidUhfATM class is a class inherited from the ATRfidUhf class and is intended to support ATM2000 and ATM500 modules.
ATRfidUhfATM(ModuleRfidUhfType, IReader) - Constructor for class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
  Create an instance of the ATRfidUhfATM class.
ATx88Reader - Class in com.atid.lib.atx88
  The ATx88Reader class inherits from the ATEAReader class and provides the common functionality of the AT188N Device, AT388 Device, and RF Prisma Device.
ATx88Reader(ATransport) - Constructor for class com.atid.lib.atx88.ATx88Reader
  Create an instance of the ATx88Reader class.
ATx88Reader(int, ATransport) - Constructor for class com.atid.lib.atx88.ATx88Reader
  Create an instance of the ATx88Reader class.
AustralianPostInterpretation - Enum in com.atid.lib.module.barcode.spc.type
  This option controls what interpretation is applied to customer fields in Australian 4-State symbols.
AustraliaPostFormat - Enum in com.atid.lib.module.barcode.ssi.type
  To select one of the following formats for Australia Post,
available() - Method in class com.atid.lib.transport.ATransport
  Returns the length of data that can be read with the read method.
available() - Method in class com.atid.lib.transport.ATransportBluetooth
available() - Method in class com.atid.lib.transport.ATransportBluetoothLe
available() - Method in class com.atid.lib.transport.ATransportUsb
AztecInverse - Enum in com.atid.lib.module.barcode.ssi.type
  This parameter sets the Aztec inverse decoder setting.

A B C D E F G H I K L M N O P Q R S T U V W