# Package com.atid.lib.module.barcode.spc.type

- Enum Summary
  Enum | Description
  --- | ---
  AustralianPostInterpretation | This option controls what interpretation is applied to customer fields in Australian 4-State symbols.
  CheckDigit | No Check Digit indicates that the scanner reads and transmits bar code data with or without a check digit.
  CodabarCheckCharacter | Codabar check characters are created using different “modulos.”
  CodabarConcatenation | Codabar supports symbol concatenation.
  Code11CheckDigitsRequired | This option sets whether 1 or 2 check digits are required with Code 11 bar codes.
  Code39CheckCharacter | No Check Character indicates that the scanner reads and transmits bar code data with or without a check character.
  CodePages | ISO 2022/ISO 646 Character Replacements Code pages define the mapping of character codes to characters.
  GS1Emulation | The scanner can automatically format the output from any GS1 data carrier to emulate what would be encoded in an equivalent GS1-128 or GS1 DataBar symbol.
  MSICheckCharacter | Different types of check characters are used with MSI bar codes.
  ResponseType | The device responds to serial commands with one of three responses: ACK (0x06) Indicates a good command which has been processed.
  TelepenOutput | Using AIM Telepen Output, the scanner reads symbols with start/stop pattern 1 and decodes them as standard full ASCII (start/stop pattern 1).
  UPCAEAN13ExtendedCouponCode | Use the following codes to enable or disable UPC-A and EAN-13 with Extended Coupon Code.
  VideoReverse | Video Reverse is used to allow the scan engine to read bar codes that are inverted.