# Package com.atid.lib.module.rfid.uhf.params

- Class Summary
  Class | Description
  --- | ---
  EpcMaskParam | The EpcMaskParam class stores information about the EPC Mask when the RFID UHF module sets or returns an EPC Mask.
  FreqTableList | The FreqTableList class represents the frequency channel information of the RFID UHF module.
  Lock6cParam | The Lock6cParam class is used to pass information that the RFID UHF's Lock command performs.
  Mask6cPattern | The Mask6cPattern class is a class that represents the Mask Pattern of a Selection Mask in terms of pattern and length.
  PermaLock6cParam | The PermaLock6cParam class is used to pass information pertaining to RFID UHF's PermaLock command.
  PowerRange | The PowerRange class is a class that represents the setting range of the power gain level of an RFID UHF antenna.
  SelectMask6cParam | The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
  TagExtParam | The TagExtParam class is a class for providing RSSI and Phase of the recognized tag as additional information if the RSSI Report property is set to true when an event occurs such as Inventory, Read Memory, Write Memory, Lock, and Kill.

- Enum Summary
  Enum | Description
  --- | ---
  Lock6cParam.LockState |
  PermaLock6cParam.LockState |