A B C D E F G H I K L M N O P Q R S T U V W

## G

get(int) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the parameter information of the barcode module.
get(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the parameter information of the barcode module.
get(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the parameter information of the barcode module.
getAccessPassword() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getAccessPassword() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device communicates with the tag, it returns the Access Password to use.
getAccessPassword() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Access Password Area of ​​Reserved Memory'.
getAccessPassword() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Access Password Area of Reserved Memory'.
getAction() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  This method is used internally by the SDK.
getAction() - Method in enum com.atid.lib.module.rfid.uhf.params.Lock6cParam.LockState
getAction() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  This method is used internally by the SDK.
getAction() - Method in enum com.atid.lib.module.rfid.uhf.params.PermaLock6cParam.LockState
getAction() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns the Action value of "Selection Mask".
getAction() - Method in class com.atid.lib.reader.ATEAReader
  Returns the current behavior of the device associated with an instance of the ATEAReader class.
getAddress() - Method in class com.atid.lib.reader.ATEAReader
  Returns the address of the device associated with an instance of the ATEAReader class.
getAddress() - Method in class com.atid.lib.transport.ATransport
  Returns the address of the device to which the ATransport instance is connected.
getAlertNotify() - Method in class com.atid.lib.atx88.ATn88Reader
getAlertNotify() - Method in class com.atid.lib.reader.ATEAReader
  Returns the alert Notify method of the instrument.
getAlgorithmType() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getAlgorithmType() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
getAt(SPCParamName) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the parameter information of the barcode module.
getAt(SSI1DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the parameter information of the barcode module.
getAt(SSI2DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the parameter information of the barcode module.
getAutoConnect() - Method in class com.atid.lib.reader.ATEAReader
  Returns whether automatically connect to the device with the instance of the ATEAReader class.
getAutoConnect() - Method in class com.atid.lib.transport.ATransport
  Returns whether automatically connect to the appliance using an instance of the Transport class.
getAutoConnect() - Method in class com.atid.lib.transport.ATransportBluetooth
getAutoConnect() - Method in class com.atid.lib.transport.ATransportBluetoothLe
getAutoConnect() - Method in class com.atid.lib.transport.ATransportUsb
getAutoOffTime() - Method in class com.atid.lib.atx88.ATx88Reader
getAutoOffTime() - Method in class com.atid.lib.reader.ATEAReader
  Returns the time at which the instrument automatically turns off.
getAutoSaveMode() - Method in class com.atid.lib.atx88.ATx88Reader
  When the device reads a tag or barcode, it returns whether to store it in the device internal memory.
getBackupState() - Method in class com.atid.lib.reader.ATEAReader
getBank() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
getBarcode() - Method in class com.atid.lib.reader.ATEAReader
  If the ATEAReader instance supports the Barcode module, it returns an interface object that can control the Barcode module.
getBarcodeParam(byte[]) - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns the parameter value to the barcode module of the instrument.
getBarcodeParamString(String) - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns the parameters of the barcode module in string format.
getBatteryState() - Method in class com.atid.lib.atx88.ATx88Reader
getBatteryState() - Method in class com.atid.lib.reader.ATEAReader
  Returns the state of the equipment.
getButtonNotify() - Method in class com.atid.lib.atx88.ATn88Reader
getButtonNotify() - Method in class com.atid.lib.reader.ATEAReader
  Returns the button Notify method of the equipment.
getButtonNotifyTime() - Method in class com.atid.lib.atx88.ATn88Reader
getButtonNotifyTime() - Method in class com.atid.lib.reader.ATEAReader
  Returns the button's Notify hold time.
getBuzzer() - Method in class com.atid.lib.atx88.ATx88Reader
getBuzzer() - Method in class com.atid.lib.reader.ATEAReader
  Returns the buzzer operation status of the equipment.
getBytes(BarcodeType[]) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(BarcodeType[], int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(BarcodeType[], int, int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(BarcodeType[], boolean[], int, int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(BarcodeType[], boolean, int, int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(SymbolStateList) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(SymbolStateList, int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(SymbolStateList, int, int) - Method in class com.atid.lib.module.barcode.ATBarcode
getBytes(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Returns the parameter value to the barcode module of the instrument.
getBytes(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the parameters of the SSI1DParamValueList.
getBytes(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Returns the parameter value to the barcode module of the instrument.
getBytes(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the parameters of the SSI2DParamValueList.
getCharset() - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns The Charset to be used to decode the Barcode data ATD100 is not supported.
getCheckInterval() - Method in class com.atid.lib.reader.ATEAReader
  Returns the time period for checking the battery status of the device associated with an instance of the ATEAReader class.
getCode() - Method in exception com.atid.lib.diagnostics.ATException
  Returns fault and motion results.
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.AustralianPostInterpretation
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.CheckDigit
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.CodabarCheckCharacter
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.CodabarConcatenation
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.Code11CheckDigitsRequired
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.Code39CheckCharacter
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.CodePages
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.GS1Emulation
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.MSICheckCharacter
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.ResponseType
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.TelepenOutput
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.UPCAEAN13ExtendedCouponCode
getCode() - Method in enum com.atid.lib.module.barcode.spc.type.VideoReverse
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.AustraliaPostFormat
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.AztecInverse
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.BooklandISBNFormat
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.CodabarStartStopCharactersDetection
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.Code11CheckDigitVerification
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.CodeLengthType
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.CompositeBeepMode
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.CouponReport
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.DataMatrixInverse
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.DecodeMirrorImages
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.DecodeUpcEanJanSupplementals
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.GS1DataBarLimitedSecurityLevel
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.HanXinInverse
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.I2of5CheckDigitVerification
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.I2of5SecurityLevel
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.IntercharacterGapSize
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.Inverse1D
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.ISBTConcatenation
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.LinearSecurityLevel
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.MSICheckDigitAlgorithm
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.MSICheckDigits
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.Preamble
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.QRInverse
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.QuietZoneLevel1D
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.RedundancyLevel
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.SecurityLevel
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.UpcCompositeMode
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.UpcEanJanSupplementalAIMIDFormat
getCode() - Method in enum com.atid.lib.module.barcode.ssi.type.UpcEanSecurityLevel
getCode() - Method in enum com.atid.lib.module.rfid.uhf.params.Lock6cParam.LockState
getCode() - Method in enum com.atid.lib.module.rfid.uhf.params.PermaLock6cParam.LockState
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.AlgorithmType
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.BankType
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.GlobalBandType
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.LinkProfileType
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.Mask6cAction
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.Mask6cTarget
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.SelectFlag
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.SessionFlag
getCode() - Method in enum com.atid.lib.module.rfid.uhf.types.SessionTarget
getCode() - Method in enum com.atid.lib.reader.types.BuzzerState
getCode() - Method in enum com.atid.lib.reader.types.CommType
getCode() - Method in enum com.atid.lib.reader.types.DataType
getCode() - Method in enum com.atid.lib.reader.types.KeyState
getCode() - Method in enum com.atid.lib.reader.types.KeyType
getCode() - Method in enum com.atid.lib.reader.types.NotificationState
getCode() - Method in enum com.atid.lib.reader.types.NotifyTimeType
getCode() - Method in enum com.atid.lib.reader.types.OperationMode
getCode() - Method in enum com.atid.lib.reader.types.UsbChargerControl
getCode() - Method in enum com.atid.lib.reader.types.UsbChargerState
getCode() - Method in enum com.atid.lib.reader.types.UsbChargerType
getCode() - Method in enum com.atid.lib.transport.types.ConnectState
getCode() - Method in enum com.atid.lib.transport.types.ConnectType
getCode() - Method in enum com.atid.lib.types.ActionState
getCode() - Method in enum com.atid.lib.types.ActionType
getCode() - Method in enum com.atid.lib.types.DeviceType
getCode() - Method in interface com.atid.lib.types.IEnumType
getCode() - Method in enum com.atid.lib.types.ModuleBarcodeProtocolType
getCode() - Method in enum com.atid.lib.types.ModuleBarcodeType
getCode() - Method in enum com.atid.lib.types.ModuleRfidHfType
getCode() - Method in enum com.atid.lib.types.ModuleRfidUhfType
getCode() - Method in enum com.atid.lib.types.ResultCode
getCommand() - Method in enum com.atid.lib.module.barcode.spc.param.SPCParamName
getCommand(int) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the parameters of the SPCParamValueList.
getCommand() - Method in enum com.atid.lib.module.barcode.ssi.param.SSI1DParamName
getCommand() - Method in enum com.atid.lib.module.barcode.ssi.param.SSI2DParamName
getConnectType() - Method in class com.atid.lib.reader.ATEAReader
  Returns the instance of ATEAReader associated with device.
getConnectType() - Method in class com.atid.lib.transport.ATransport
  Returns the instance of Transport associated with device.
getContinuousMode() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getContinuousMode() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns whether the RFID UHF module on the device will cause the Inventory to run continuously.
getCount() - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Returns the type of symbol stored in the SymbolStateList instance and the number of pieces of information in the state pair.
getCount() - Method in class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Returns the type of parameter stored in the SPCParamNameList instance.
getCount() - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the type of parameter stored in the SPCParamValueList instance and the number of pieces of information in the value pair.
getCount() - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Returns the type of parameter stored in the SSI1DParamNameList instance.
getCount() - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the type of parameter stored in the SSI1DParamValueList instance and the number of pieces of information in the value pair.
getCount() - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Returns the type of parameter stored in the SSI2DParamNameList instance.
getCount() - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the type of parameter stored in the SSI2DParamValueList instance and the number of pieces of information in the value pair.
getCount() - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Returns the number of channels stored in the FreqTableList instance.
getCurrentLinkProfile() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getCurrentLinkProfile() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the link profile of the RFID UHF module of the Device. ( Temporarily Type )
getData() - Method in class com.atid.lib.reader.params.StoredDataList.StoredData
  Returns data for a StoredData instance.
getDefaultLinkProfile() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getDefaultLinkProfile() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the link profile of the RFID UHF module of the Device. ( Permanently Type ) The power of the device must be turned off and on.
getDeviceAttached() - Method in class com.atid.lib.reader.ATEAReader
  Returns whether attached to the device with the instance of the ATEAReader class..
getDeviceAttached() - Method in class com.atid.lib.transport.ATransport
  Returns whether attached to the appliance using an instance of the Transport class.
getDeviceAttached() - Method in class com.atid.lib.transport.ATransportBluetooth
getDeviceAttached() - Method in class com.atid.lib.transport.ATransportBluetoothLe
getDeviceAttached() - Method in class com.atid.lib.transport.ATransportUsb
getDeviceName() - Method in class com.atid.lib.reader.ATEAReader
  Returns the name of the Device associated with an instance of the ATEAReader class.
getDeviceName() - Method in class com.atid.lib.transport.ATransport
  Returns the name of the Device to which the ATransport instance is connected.
getDeviceType() - Method in class com.atid.lib.reader.ATEAReader
  ATEAReader Returns the type of Device to which the instance is connected.
getDeviceType() - Method in class com.atid.lib.transport.ATransport
  ATransport Returns the type of device to which the instance will be connected.
getDisplayOffTime() - Method in class com.atid.lib.atx88.ATx88Reader
  Returns the time to turn off the display automatically when the device is not in use.
getEpc() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpc() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'EPC memory'.
getEpcMask(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getEpcMask(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the EPC Mask of the RFID UHF module of the Device.
getEpcMaskCount() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getEpcMaskCount() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the number of EPC Mask items in the RFID UHF module of the device.
getEpcMaskMatchMode() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getEpcMaskMatchMode() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the method of comparing the EPC Mask items of the RFID UHF module of the Device.
getFreqName(int) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  FreqTableList Returns the frequency value obtained by converting the channel stored in the instance into Unit units.
getFreqNames() - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  FreqTableList Returns the frequency value obtained by converting the channel of all channel information stored in the instance into Unit unit.
getFreqTable() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getFreqTable() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the Device returns the frequency table.
getFrequency(int) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Returns the frequency value of the channel stored in the FreqTableList instance.
getFrequency() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Frequency value of the tag. ( Unit : MHz )
getFrequencyD() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Frequency value of the tag. ( Unit : MHz )
getFrequencyRaw() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Frequency value of the tag. ( Unit : MHz )
getFullVersionHexa() - Method in class com.atid.lib.reader.ATEAReader
  Returns the hw & firmware version of the device associated with the instance of the ATEAReader class.
getGlobalBand() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getGlobalBand() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the national orientation of the RFID UHF module of the instrument.
getIdleTime() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getIdleTime() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the instrument returns the time that the radio waves are not output in the Inventory operation and is resting.
getInventoryTagType() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getInventoryTagType() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs an inventory operation, it returns the type of Inventory tags.
getInventoryTime() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getInventoryTime() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the time at which radio waves are actually output from the Inventory operation of the RFID UHF module in the instrument.
getKillPassword() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Returns TAG Access operation for 'Kill Password Area of ​​Reserved Memory'.
getKillPassword() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Returns TAG Access operation for 'Kill Password Area of Reserved Memory'.
getLastError() - Method in class com.atid.lib.reader.ATEAReader
getLength() - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Returns the Length of the EpcMaskParam instance.
getLength() - Method in class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Returns the pattern length of the Mask6cPattern instance.
getLength() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns the Length value of "Selection Mask".
getLength1() - Method in class com.atid.lib.module.barcode.ssi.type.CodeLength
getLength2() - Method in class com.atid.lib.module.barcode.ssi.type.CodeLength
getLengthType() - Method in class com.atid.lib.module.barcode.ssi.type.CodeLength
getLimitTagCount() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getLimitTagCount() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs an inventory operation, it returns the number of tags read as the stop condition of Inventory.
getLock() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  This method is used internally by the SDK.
getMacAddress() - Method in class com.atid.lib.transport.ATransport
  Returns the MAC address of the device to which the ATransport instance is connected.
getMask() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  This method is used internally by the SDK.
getMask() - Method in enum com.atid.lib.module.rfid.uhf.params.Lock6cParam.LockState
getMask() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  This method is used internally by the SDK.
getMask() - Method in enum com.atid.lib.module.rfid.uhf.params.PermaLock6cParam.LockState
getMax() - Method in class com.atid.lib.module.rfid.uhf.params.PowerRange
  Returns the maximum Power Gian Level value for a PowerRange instance.
getMaxQ() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getMaxQ() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the maximum Q value.
getMessage() - Method in enum com.atid.lib.reader.types.NotificationState
getMessage() - Method in enum com.atid.lib.types.ResultCode
getMethod(int) - Method in class com.atid.lib.reader.params.NotifyMethod
  Returns whether the notification status at the specified index.
getMin() - Method in class com.atid.lib.module.rfid.uhf.params.PowerRange
  Returns the Power Gian Level minimum value for a PowerRange instance.
getMinQ() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getMinQ() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, it returns the minimum Q value.
getName() - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Returns the type of parameter stored in the SPCParamValue instance.
getName() - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValue
  Returns the type of parameter stored in the SSI1DParamValue instance.
getName() - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValue
  Returns the type of parameter stored in the SSI2DParamValue instance.
getName(int) - Method in class com.atid.lib.reader.params.NotifyMethod
  Returns the name of the notification method at the specified index as a string.
getOffset() - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Returns the offset of the EpcMaskParam instance.
getOffset() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns the Offset value of "Selection Mask".
getOperationMode() - Method in class com.atid.lib.atx88.ATx88Reader
getOperationMode() - Method in class com.atid.lib.reader.ATEAReader
  Returns the current operating mode of the instrument.
getOperationTime() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getOperationTime() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the operating time of the RFID UHF module of the instrument.
getPattern() - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Returns Pettern of the EpcMaskParam instance.
getPattern() - Method in class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Returns the Mask pattern of the Mask6cPattern instance.
getPattern() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns the Pattern value of "Selection Mask".
getPermalock() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  This method is used internally by the SDK.
getPhase() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Phase value of the tag.
getPhaseD() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Phase value of the tag.
getPhaseRaw() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the Phase value of the tag.
getPower() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getPower() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the antenna output of the RFID UHF module of the instrument.
getPowerRange() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getPowerRange() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the antenna output range of the RFID UHF module of the instrument.
getProtocol() - Method in class com.atid.lib.reader.ATEAReader
getQueryCommand(int) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Returns the parameter names of the barcode module.
getReadTidLength() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getReadTidLength() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device returns the length of TID memory that can be read along with Tag value at Inventory for TID Inventory when TID Inventory function is supported.
getReportMode() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getReportMode() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Inventory the device as an RFID UHF module and return whether the tag read will send the same tag to the event only once or read each time it is read.
getReportRssi() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getReportRssi() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns whether the RFID UHF module of the device will pass additional RSSI and Phase to the operation result.
getResponse() - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Returns the result of parameter stored in the SPCParamValue instance.
getRfidHf() - Method in class com.atid.lib.reader.ATEAReader
  If the ATEAReader instance supports the RFID HF module, it returns an interface object that can control the RFID HF module.
getRfidUhf() - Method in class com.atid.lib.reader.ATEAReader
  If the ATEAReader instance supports the RFID UHF module, it returns an interface object that can control the RFID UHF module.
getRssi() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the RSSI value of the tag.
getRssiD() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the RSSI value of the tag.
getRssiRaw() - Method in class com.atid.lib.module.rfid.uhf.params.TagExtParam
  Returns the RSSI value of the tag.
getSameTagReportTime() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSameTagReportTime() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs an Inventory operation, it returns the time when the same tag is not recognized again.
getSelectFlag() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectFlag() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the device returns the status of the Select Flag of the tag to be read by the Inventory operation.
getSelectMask6c(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6c(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cAction(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cAction(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the comparison behavior of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cBank(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cBank(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The Selection Mask item of the Device's RFID UHF module returns the memory bank to compare.
getSelectMask6cEnabled(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cEnabled(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns whether to use the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cOffset(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cOffset(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The Selection Mask item of the RFID UHF module of the Device returns the starting address of the memory to start the comparison.
getSelectMask6cPattern(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cPattern(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the comparison value and length of the Selection Mask item of the RFID UHF module of the Device.
getSelectMask6cTarget(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSelectMask6cTarget(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the Flag of the tag to store the comparison result of Selection Mask item of RFID UHF module of Device.
getSerialNo() - Method in class com.atid.lib.atx88.ATx88Reader
getSerialNo() - Method in class com.atid.lib.reader.ATEAReader
  Returns the serial number of the device.
getSessionFlag() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSessionFlag() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the device returns the status of the Session Flag of the tag to be read by the Inventory operation.
getSessionId() - Method in class com.atid.lib.reader.ATEAReader
  Returns the Session ID of the ATEAReader instance.
getSessionTarget() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getSessionTarget() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the device returns the Session Flag to check the state of the Session Flag of the tag to be read by the Inventory operation.
getSlot(int) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Returns the slot of the channel stored in the FreqTableList instance.
getStartQ() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getStartQ() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, it returns the starting Q value.
getState() - Method in class com.atid.lib.reader.ATEAReader
  Returns the connection status of the device with the instance of the ATEAReader class.
getState() - Method in class com.atid.lib.transport.ATransport
  The instance of ATransport returns the connection status with device.
getStoredTagCount() - Method in class com.atid.lib.atx88.ATx88Reader
getStoredTagCount() - Method in class com.atid.lib.reader.ATEAReader
  Returns the number of data stored in the device's internal memory.
getString(BarcodeType[]) - Method in class com.atid.lib.module.barcode.ATBarcode
getSymbolPostState() - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns the post office symbol set in the barcode module.
getSymbolState() - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns the status of all symbols in the barcode module.
getSymbolState(byte[]) - Method in class com.atid.lib.module.barcode.ATBarcode
getTable() - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Returns whether to use frequency channel in bit wise form.
getTarget() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns the Target Flag of "Selection Mask".
getTid() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Returns TAG Access action for 'TID memory'.
getTid() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Returns TAG Access action for 'TID memory'.
getTime() - Method in class com.atid.lib.atx88.ATx88Reader
getTime() - Method in class com.atid.lib.reader.ATEAReader
  Returns the system time of the device.
getTransport() - Method in class com.atid.lib.reader.ATEAReader
  Returns an instance of the ATransport class that connects an instance of the ATEAReader class to the Device.
getType() - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns the Barcode module type of the connected device.
getType(int) - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Returns the barcode type at the specified index.
getType() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the RFID UHF module type of the connected Device.
getType() - Method in class com.atid.lib.reader.params.StoredDataList.StoredData
  Returns the data type of the StoredData instance.
getUnlock() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  This method is used internally by the SDK.
getUseActionKey() - Method in class com.atid.lib.atx88.ATx88Reader
getUseActionKey() - Method in class com.atid.lib.reader.ATEAReader
  Returns whether to use the action of the Trigger button on the instrument.
getUsed(int) - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Returns the status of the bar code symbol at the specified index.
getUser() - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Returns TAG Access action for 'EPC memory'.
getUser() - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Returns TAG Access behavior for 'User memory'.
getValue() - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Returns the value of parameter stored in the SPCParamValue instance.
getValue(int) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the parameter value of the SPCParamValueList.
getValue() - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValue
  Returns the value of parameter stored in the SSI1DParamValue instance.
getValue(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the parameter value of the SSI1DParamValueList.
getValue() - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValue
  Returns the value of parameter stored in the SSI2DParamValue instance.
getValue(int) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the parameter value of the SSI2DParamValueList.
getValue() - Method in class com.atid.lib.reader.params.NotifyMethod
  Returns the notification state in bit wise format.
getValueAt(SPCParamName) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Returns the parameter value of the SPCParamValueList.
getValueAt(SSI1DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Returns the parameter value of the SSI1DParamValueList.
getValueAt(SSI2DParamName) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Returns the parameter value of the SSI2DParamValueList.
getVersion() - Method in class com.atid.lib.module.barcode.ATBarcode
  The Barcode module returns the version.
getVersion() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
getVersion() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Returns the version of the RFID UHF module.
getVersion() - Method in class com.atid.lib.reader.ATEAReader
  Returns the firmware version of the device associated with the instance of the ATEAReader class.
getVersionHexa() - Method in class com.atid.lib.reader.ATEAReader
  Returns the firmware version of the device associated with the instance of the ATEAReader class.
GlobalBandType - Enum in com.atid.lib.module.rfid.uhf.types
  The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.
GS1DataBarLimitedSecurityLevel - Enum in com.atid.lib.module.barcode.ssi.type
  The decoder offers four levels of decode security for GS1 DataBar Limited bar codes.
GS1Emulation - Enum in com.atid.lib.module.barcode.spc.type
  The scanner can automatically format the output from any GS1 data carrier to emulate what would be encoded in an equivalent GS1-128 or GS1 DataBar symbol.

A B C D E F G H I K L M N O P Q R S T U V W