A B C D E F G H I K L M N O P Q R S T U V W

## I

I2of5CheckDigitVerification - Enum in com.atid.lib.module.barcode.ssi.type
  Enable this feature to check the integrity of all I 2 of 5 symbols to verify the data complies with either the specified Uniform Symbology Specification (USS), or the Optical Product Code Council (OPCC) check digit algorithm.
I2of5SecurityLevel - Enum in com.atid.lib.module.barcode.ssi.type
  Interleaved 2 of 5 bar codes are vulnerable to misdecodes by the nature of the symbol, especially when Any Length is set for Interleaved 2 of 5 bar codes.
IATBarcodeEventListener - Interface in com.atid.lib.module.barcode.event
  IATBarcodeEventListener interface is an interface for handling events raised by the barcode module.
IATEAReaderEventListener - Interface in com.atid.lib.reader.event
  ATEAReader Interface for passing events to an application when an event occurs in the instance.
IATRfidUhfEventListener - Interface in com.atid.lib.module.rfid.uhf.event
  The IATRfidUhfEventListener interface is an interface that defines event handling methods for handling events raised by the ATRfidUhf instance.
IEnumType - Interface in com.atid.lib.types
  The IEnumType interface provides the common functionality of all enumerations that the SDK uses.
INFO - Static variable in class com.atid.lib.module.barcode.ATBarcode
INFO - Static variable in class com.atid.lib.module.rfid.uhf.ATRfidUhf
INFO - Static variable in class com.atid.lib.reader.ATEAReader
INFO - Static variable in class com.atid.lib.transport.ATransport
initMoudle() - Method in class com.atid.lib.module.barcode.ATBarcode
  After the Device is connected, it calls to instantiate the ATBarcode instance.
initMoudle() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
initMoudle() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  After the Device is connected, it calls to instantiate the ATRfidUhf instance.
initReader() - Method in class com.atid.lib.atx88.ATx88Reader
initReader() - Method in class com.atid.lib.reader.ATEAReader
  Initializes an ATEAReader instance after the ATEAReader instance is associated with the device.
IntercharacterGapSize - Enum in com.atid.lib.module.barcode.ssi.type
  The Code 39 and Codabar symbologies have an intercharacter gap that is typically quite small.
inventory6b() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
inventory6b() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to inventory the RFID UHF tag of ISO18000-6c Gen2 standard.
inventory6c() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
inventory6c() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device instructs to inventory the RFID UHF tag of ISO18000-6c Gen2 standard.
Inverse1D - Enum in com.atid.lib.module.barcode.ssi.type
  This parameter sets the 1D inverse decoder setting.
IO - Static variable in class com.atid.lib.transport.ATransport
ISBTConcatenation - Enum in com.atid.lib.module.barcode.ssi.type
  Select an option for concatenating pairs of ISBT code types
isEmptyRef() - Method in class com.atid.lib.reader.ATEAReader
  Checks if an instance of the ATEAReader class is currently being referenced.
isSuportSelPost() - Method in class com.atid.lib.module.barcode.ATBarcode
  Returns whether the barcode module can select the post office symbol.
isUsed(int) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Returns whether the frequency channel stored in the FreqTableList instance is used.
isUsed() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Returns whether or not "Selection Mask" is enabled.

A B C D E F G H I K L M N O P Q R S T U V W