A B C D E F G H I K L M N O P Q R S T U V W

## U

UPCAEAN13ExtendedCouponCode - Enum in com.atid.lib.module.barcode.spc.type
  Use the following codes to enable or disable UPC-A and EAN-13 with Extended Coupon Code.
UpcCompositeMode - Enum in com.atid.lib.module.barcode.ssi.type
  If you enable Composite CC-A/B , select an option for linking UPC symbols with a 2D symbol during transmission as if they were one symbol
UpcEanJanSupplementalAIMIDFormat - Enum in com.atid.lib.module.barcode.ssi.type
  Select an output format when reporting UPC/EAN/JAN bar codes with Supplementals with Transmit Code ID Character set to AIM Code ID Character:
UpcEanSecurityLevel - Enum in com.atid.lib.module.barcode.ssi.type
  The 1D Barcode Scanner offers four levels of decode security for UPC/EAN bar codes.
UsbChargerControl - Enum in com.atid.lib.reader.types
  The UsbChargerType enumeration specifies whether to connect or disconnect a device connected to the USB port on the device.
UsbChargerState - Enum in com.atid.lib.reader.types
  The UsbChargerState enumeration represents the usb charging of the Device.
UsbChargerType - Enum in com.atid.lib.reader.types
  The UsbChargerType enumeration represents a device connected to the device's USB port.

A B C D E F G H I K L M N O P Q R S T U V W