A B C D E F G H I K L M N O P Q R S T U V W

## S

saveStoredData(StoredDataList) - Method in class com.atid.lib.atx88.ATx88Reader
saveStoredData(StoredDataList) - Method in class com.atid.lib.reader.ATEAReader
  Store tag data or barcode data on the instrument.
SecurityLevel - Enum in com.atid.lib.module.barcode.ssi.type
  The decoder offers four levels of decode security for delta bar codes, which include UPC/EAN and Code 93.
SelectFlag - Enum in com.atid.lib.module.rfid.uhf.types
  The SelectFlag enumeration represents the status of the Select Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
SelectMask6cParam - Class in com.atid.lib.module.rfid.uhf.params
  The SelectMask6cParam class is a class for providing the capability to set Selection Mask conditions on RFID UHF modules at once.
SelectMask6cParam() - Constructor for class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, String, int) - Constructor for class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SelectMask6cParam(boolean, Mask6cTarget, Mask6cAction, BankType, int, <any>) - Constructor for class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Creates an instance of the SelectMask6cParam class.
SessionFlag - Enum in com.atid.lib.module.rfid.uhf.types
  The SessionFlag enumeration type indicates the status of the Session Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
SessionTarget - Enum in com.atid.lib.module.rfid.uhf.types
  The SessionTarget enumeration represents the Session Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
setAccessPassword(String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setAccessPassword(String) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the Access Password to use when the RFID UHF module of the device communicates with the tag.
setAccessPassword(Lock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Set TAG Access operation for 'Access Password Area of ​​Reserved Memory'.
setAccessPassword(PermaLock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Access Password Area of Reserved Memory'.
setAction(ActionState, String) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setAction(Mask6cAction) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Action value of "Selection Mask".
setAction(ActionState) - Method in class com.atid.lib.reader.ATEAReader
  ATEAReader Sets the operational state of the device associated with the instance.
setAddress(String) - Method in class com.atid.lib.reader.ATEAReader
  Sets the address of the device to which the instance of ATEAReader is connected.
setAddress(String) - Method in class com.atid.lib.transport.ATransport
  Sets the address of the device to which the ATransport instance is connected.
setAlertNotify(NotifyMethod) - Method in class com.atid.lib.atx88.ATn88Reader
setAlertNotify(NotifyMethod) - Method in class com.atid.lib.reader.ATEAReader
  Set the alert notify method for the device.
setAlgorithmType(AlgorithmType) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setAlgorithmType(AlgorithmType) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets the algorithm that the RFID UHF module of the appliance uses to perform the inventory.
setAutoConnect(boolean) - Method in class com.atid.lib.reader.ATEAReader
  Sets whether automatically connect to the device with the instance of the ATEAReader class.
setAutoConnect(boolean) - Method in class com.atid.lib.transport.ATransport
  Sets whether automatically connect to the appliance using an instance of the Transport class.
setAutoConnect(boolean) - Method in class com.atid.lib.transport.ATransportBluetooth
setAutoConnect(boolean) - Method in class com.atid.lib.transport.ATransportBluetoothLe
setAutoConnect(boolean) - Method in class com.atid.lib.transport.ATransportUsb
setAutoOffTime(int) - Method in class com.atid.lib.atx88.ATx88Reader
setAutoOffTime(int) - Method in class com.atid.lib.reader.ATEAReader
  Sets the time at which the equipment automatically turns off.
setAutoSaveMode(boolean) - Method in class com.atid.lib.atx88.ATx88Reader
  When the device reads a tag or barcode, it sets whether or not to store it in the internal memory of the device.
setBank(BankType) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Bank value in "Selection Mask".
setBarcodeParam(byte[]) - Method in class com.atid.lib.module.barcode.ATBarcode
  Set the parameter value on the barcode module of the machine.
setBarcodeParamString(String) - Method in class com.atid.lib.module.barcode.ATBarcode
  Sets the parameters of the barcode module in string format.
setBufferControlListener(int, ATransport.IBufferControlEventListener) - Method in class com.atid.lib.transport.ATransport
  Sets the listener to be notified of buffer status in order for an instance of the Transport class to dynamically control the buffer.
setBufferControlListener(int, int, ATransport.IBufferControlEventListener) - Method in class com.atid.lib.transport.ATransport
  Sets the listener to be notified of buffer status in order for an instance of the Transport class to dynamically control the buffer.
setButtonNotify(NotifyMethod) - Method in class com.atid.lib.atx88.ATn88Reader
setButtonNotify(NotifyMethod) - Method in class com.atid.lib.reader.ATEAReader
  Set the button Notify method of the device.
setButtonNotifyTime(NotifyTimeType) - Method in class com.atid.lib.atx88.ATn88Reader
setButtonNotifyTime(NotifyTimeType) - Method in class com.atid.lib.reader.ATEAReader
  Set the button's Notify hold time.
setBuzzer(BuzzerState) - Method in class com.atid.lib.atx88.ATx88Reader
setBuzzer(BuzzerState) - Method in class com.atid.lib.reader.ATEAReader
  Sets the buzzer operation status of the equipment.
setCharset(Charset) - Method in class com.atid.lib.module.barcode.ATBarcode
  Sets The Charset to be used to decode the Barcode data.
setCheckInterval(int) - Method in class com.atid.lib.reader.ATEAReader
  Sets the time period for checking the battery status of the device associated with the ATEAReader class instance.
setContinuousMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setContinuousMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets whether or not the RFID UHF module of the device will run the Inventory continuously.
setCurrentLinkProfile(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setCurrentLinkProfile(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets the link profile of the RFID UHF module of the Device. ( Temporarily Type )
setData(String) - Method in class com.atid.lib.reader.params.StoredDataList.StoredData
  Sets the data for the StoredData instance.
setDefaultLinkProfile(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setDefaultLinkProfile(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets the link profile of the RFID UHF module of the Device. ( Permanently Type ) The power of the device must be turned off and on.
setDeviceName(String) - Method in class com.atid.lib.reader.ATEAReader
  Sets the name of the device to which the instance of ATEAReader is connected.
setDeviceName(String) - Method in class com.atid.lib.transport.ATransport
  Sets the name of the device to which the ATransport instance is connected.
setDeviceType(DeviceType) - Method in class com.atid.lib.reader.ATEAReader
  Sets the type of device to which instance of ATEAReader will be connected.
setDeviceType(DeviceType) - Method in class com.atid.lib.transport.ATransport
  ATransport Sets the type of device to which the instance will be connected.
setDisplayOffTime(int) - Method in class com.atid.lib.atx88.ATx88Reader
  Sets the time to turn off the display automatically when not using the device.
setEpc(Lock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setEpc(PermaLock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Set TAG Access action for 'EPC memory'.
setEpcMaskMatchMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setEpcMaskMatchMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the method of comparing EPC Mask items of the RFID UHF module of the device.
setException(ATException) - Method in class com.atid.lib.module.barcode.ATBarcode
setException(ATException) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setForceBatteryGauging(boolean) - Method in class com.atid.lib.reader.ATEAReader
  Sets whether check battery status of the device during action associated with the ATEAReader class instance.
setFreqTable(FreqTableList) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setFreqTable(FreqTableList) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the device sets up the frequency table.
setFrequency(int, int) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Sets the frequency value of the channel stored in the FreqTableList instance.
setGlobalBand(GlobalBandType) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setGlobalBand(GlobalBandType) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the national orientation of the RFID UHF module of the instrument.
setIdleTime(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setIdleTime(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the instrument sets the time for which the radio waves are not output in the Inventory operation and the rest of the time.
setInventoryTagType(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setInventoryTagType(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs the inventory operation, it sets the specified type of the tags Inventory.
setInventoryTime(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setInventoryTime(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets the time at which radio waves are actually output in Inventory operation of the RFID UHF module of the instrument.
setKillPassword(Lock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Set TAG Access operation for 'Kill Password Area of ​​Reserved Memory'.
setKillPassword(PermaLock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'Kill Password Area of Reserved Memory'.
setLastError(ResultCode) - Method in class com.atid.lib.reader.ATEAReader
setLength(int, int) - Method in class com.atid.lib.module.barcode.ssi.type.CodeLength
setLength(int) - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Sets the Length of the EpcMaskParam instance.
setLength(int) - Method in class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Sets the pattern length of the Mask6cPattern instance.
setLength(int) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Length value of "Selection Mask".
setLengthType(CodeLengthType) - Method in class com.atid.lib.module.barcode.ssi.type.CodeLength
setLimitTagCount(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setLimitTagCount(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs the inventory operation, it sets the number of tags read as the stop condition of Inventory.
setMacAddress(String) - Method in class com.atid.lib.transport.ATransport
  Sets the MAC address of the device to which the ATransport instance is connected.
setMax(int) - Method in class com.atid.lib.module.rfid.uhf.params.PowerRange
  Sets the maximum Power Gian Level value for a PowerRange instance.
setMaxQ(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setMaxQ(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the maximum Q value.
setMethods(int, boolean) - Method in class com.atid.lib.reader.params.NotifyMethod
  Sets whether or not to be notified at the specified index.
setMin(int) - Method in class com.atid.lib.module.rfid.uhf.params.PowerRange
  Sets the Power Gian Level minimum value for a PowerRange instance.
setMinQ(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setMinQ(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device uses Dynamic Q, set the minimum Q value.
setOffset(int) - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Sets the offset of the EpcMaskParam instance.
setOffset(int) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Offset value of "Selection Mask".
setOperationMode(OperationMode) - Method in class com.atid.lib.atx88.ATx88Reader
setOperationMode(OperationMode) - Method in class com.atid.lib.reader.ATEAReader
  Sets the current operating mode of the instrument.
setOperationTime(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setOperationTime(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the operation time of the RFID UHF module of the device.
setPattern(String) - Method in class com.atid.lib.module.rfid.uhf.params.EpcMaskParam
  Sets the Pettern for the EpcMaskParam instance.
setPattern(String) - Method in class com.atid.lib.module.rfid.uhf.params.Mask6cPattern
  Mask6cPattern Sets the Mask pattern for the instance.
setPattern(String) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Pattern value of "Selection Mask".
setPower(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setPower(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the antenna output of the RFID UHF module of the instrument.
setReadTidLength(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setReadTidLength(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the TID Inventory function is supported by the device, set the TID memory length that can be read along with the Tag value at the time of Inventory for TID Inventory.
setReportMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setReportMode(boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Inventory the device as an RFID UHF module and set whether the read tag sends the same tag to the event only once or whenever it reads it.
setReportRssi(boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setReportRssi(boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Sets whether the RFID UHF module of the device will pass additional RSSI and Phase to the operation result.
setResponse(ResponseType) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Set the result of parameter on the SPCParamValue instance.
setRfidCarrierWave(boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setRfidCarrierWave(boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs the inventory operation, it sets the specified type of the tags Inventory.
setSameTagReportTime(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSameTagReportTime(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  When the RFID UHF module of the device performs an Inventory operation, set the time at which the same tag is not recognized again.
setSelectFlag(SelectFlag) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectFlag(SelectFlag) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The RFID UHF module of the device sets the status of the Select Flag of the tag to be read by the Inventory operation.
setSelectMask6c(int, SelectMask6cParam) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6c(int, SelectMask6cParam) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cAction(int, Mask6cAction) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cAction(int, Mask6cAction) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the comparison behavior of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cBank(int, BankType) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cBank(int, BankType) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The Selection Mask item of the RFID UHF module of the device sets the memory bank to be compared.
setSelectMask6cEnabled(int, boolean) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cEnabled(int, boolean) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set whether or not to use the Selection Mask item of the RFID UHF module of the Device.
setSelectMask6cOffset(int, int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cOffset(int, int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  The Selection Mask item of the RFID UHF module of the device sets the start address of the memory to start the comparison.
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cPattern(int, Mask6cPattern) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the comparison value and length of the Selection Mask item of the RFID UHF module of the device.
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSelectMask6cTarget(int, Mask6cTarget) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Set the Flag of the tag to save the comparison result of Selection Mask item of the RFID UHF module of the device.
setSerialNo(String) - Method in class com.atid.lib.atx88.ATx88Reader
setSerialNo(String) - Method in class com.atid.lib.reader.ATEAReader
  Set the serial number of the device.
setSessionFlag(SessionFlag) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSessionFlag(SessionFlag) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device's RFID UHF module sets the state of Session flag of tag to read by Inventory operation.
setSessionTarget(SessionTarget) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setSessionTarget(SessionTarget) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Device's RFID UHF module sets the Session Flag to check the status of the Session Flag of the tag to be read by Inventory operation.
setStartQ(int) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
setStartQ(int) - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  If the algorithm of the RFID UHF module of the device is using Dynamic Q, set the starting Q value.
setState(ConnectState, Object) - Method in class com.atid.lib.transport.ATransport
setStateListener(ATransport.IConnectStateEventListener) - Method in class com.atid.lib.transport.ATransport
  Sets the listener to receive the connection status of an instance of the ATransport class.
setSymbolPostState(BarcodePostType) - Method in class com.atid.lib.module.barcode.ATBarcode
  Set the post office symbol in the bar code module.
setSymbolState(SymbolStateList) - Method in class com.atid.lib.module.barcode.ATBarcode
  Sets the symbol status of the barcode module.
setTarget(Mask6cTarget) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set the Target Flag of "Selection Mask".
setTid(Lock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Set TAG Access operation for 'TID memory'.
setTid(PermaLock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Set TAG Access operation for 'TID memory'.
setTime(Date) - Method in class com.atid.lib.atx88.ATx88Reader
setTime(Date) - Method in class com.atid.lib.reader.ATEAReader
  Sets the system time of the instrument.
setType(DataType) - Method in class com.atid.lib.reader.params.StoredDataList.StoredData
  Sets the data type of the StoredData instance.
setUsbChargingPhone(UsbChargerControl) - Method in class com.atid.lib.atx88.ATx88Reader
  Set whether or not to enable charging the phone. ( USB communication will be lost when charging the phone. ) Only ATS100 is supported.
setUseActionKey(boolean) - Method in class com.atid.lib.atx88.ATx88Reader
setUseActionKey(boolean) - Method in class com.atid.lib.reader.ATEAReader
  Set whether or not to use the operation of the Trigger button of the equipment.
setUsed(int, boolean) - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Sets the state of the bar code symbol at the specified index.
setUsed(int, boolean) - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  Sets whether to use the frequency channel stored in the FreqTableList instance.
setUsed(boolean) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Set whether or not to use "Selection Mask".
setUser(Lock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.Lock6cParam
  Set TAG Access action for 'EPC memory'.
setUser(PermaLock6cParam.LockState) - Method in class com.atid.lib.module.rfid.uhf.params.PermaLock6cParam
  Set TAG Access behavior for 'User memory'.
setValue(Object) - Method in class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Set the parameter value on the SPCParamValue instance.
setValue(Object) - Method in class com.atid.lib.module.barcode.ssi.param.SSI1DParamValue
  Set the parameter value on the SSI1DParamValue instance.
setValue(Object) - Method in class com.atid.lib.module.barcode.ssi.param.SSI2DParamValue
  Set the parameter value on the SSI2DParamValue instance.
setValue(int) - Method in class com.atid.lib.reader.params.NotifyMethod
  Sets the notification state to bit wise format.
sleep() - Method in class com.atid.lib.atx88.ATx88Reader
sleep(IATEAReaderEventListener) - Method in class com.atid.lib.atx88.ATx88Reader
sleep() - Method in class com.atid.lib.reader.ATEAReader
  An instance of the ATEAReader class is called before an active Host device goes to sleep.
sleep(IATEAReaderEventListener) - Method in class com.atid.lib.reader.ATEAReader
  An instance of the ATEAReader class is called before an active Host device goes to sleep.
sort() - Method in class com.atid.lib.module.rfid.uhf.params.FreqTableList
  FreqTableList Arrange the frequency channel information stored in the instance based on the frequency value.
SPCParamName - Enum in com.atid.lib.module.barcode.spc.param
  SPC 2D barcode module parameters.
SPCParamNameList - Class in com.atid.lib.module.barcode.spc.param
  Get data of barcode scanner's parameters.
SPCParamNameList() - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Create an instance of the SPCParamNameList class.
SPCParamNameList(SPCParamName) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Create an instance of the SPCParamNameList class.
SPCParamNameList(SPCParamName[]) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamNameList
  Create an instance of the SPCParamNameList class.
SPCParamValue - Class in com.atid.lib.module.barcode.spc.param
  Set data of barcode scanner's parameters.
SPCParamValue(SPCParamName) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Create an instance of the SPCParamValue class.
SPCParamValue(SPCParamName, Object) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Create an instance of the SPCParamValue class.
SPCParamValue(SPCParamName, Object, ResponseType) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValue
  Create an instance of the SPCParamValue class.
SPCParamValueList - Class in com.atid.lib.module.barcode.spc.param
  Get or Set data of barcode scanner's parameters.
SPCParamValueList() - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Create an instance of the SPCParamValueList class.
SPCParamValueList(SPCParamValue) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Create an instance of the SPCParamValueList class.
SPCParamValueList(SPCParamValue[]) - Constructor for class com.atid.lib.module.barcode.spc.param.SPCParamValueList
  Create an instance of the SPCParamValueList class.
SSI1DParamName - Enum in com.atid.lib.module.barcode.ssi.param
  SSI 1D barcode module parameters.
SSI1DParamNameList - Class in com.atid.lib.module.barcode.ssi.param
  Get data of barcode scanner's parameters.
SSI1DParamNameList() - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Create an instance of the SSI1DParamNameList class.
SSI1DParamNameList(SSI1DParamName) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Create an instance of the SSI1DParamNameList class.
SSI1DParamNameList(SSI1DParamName[]) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamNameList
  Create an instance of the SSI1DParamNameList class.
SSI1DParamValue - Class in com.atid.lib.module.barcode.ssi.param
  Set data of barcode scanner's parameters.
SSI1DParamValue(SSI1DParamName) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamValue
  Create an instance of the SSI1DParamValue class.
SSI1DParamValue(SSI1DParamName, Object) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamValue
  Create an instance of the SSI1DParamValue class.
SSI1DParamValueList - Class in com.atid.lib.module.barcode.ssi.param
  Get or Set data of barcode scanner's parameters.
SSI1DParamValueList() - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Create an instance of the SSI1DParamValueList class.
SSI1DParamValueList(SSI1DParamValue) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Create an instance of the SSI1DParamValueList class.
SSI1DParamValueList(SSI1DParamValue[]) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI1DParamValueList
  Create an instance of the SSI1DParamValueList class.
SSI2DParamName - Enum in com.atid.lib.module.barcode.ssi.param
  SSI 2D barcode module parameters.
SSI2DParamNameList - Class in com.atid.lib.module.barcode.ssi.param
  Get data of barcode scanner's parameters.
SSI2DParamNameList() - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Create an instance of the SSI2DParamNameList class.
SSI2DParamNameList(SSI2DParamName) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Create an instance of the SSI2DParamNameList class.
SSI2DParamNameList(SSI2DParamName[]) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamNameList
  Create an instance of the SSI2DParamNameList class.
SSI2DParamValue - Class in com.atid.lib.module.barcode.ssi.param
  Set data of barcode scanner's parameters.
SSI2DParamValue(SSI2DParamName) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamValue
  Create an instance of the SSI2DParamValue class.
SSI2DParamValue(SSI2DParamName, Object) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamValue
  Create an instance of the SSI2DParamValue class.
SSI2DParamValueList - Class in com.atid.lib.module.barcode.ssi.param
  Get or Set data of barcode scanner's parameters.
SSI2DParamValueList() - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Create an instance of the SSI2DParamValueList class.
SSI2DParamValueList(SSI2DParamValue) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Create an instance of the SSI2DParamValueList class.
SSI2DParamValueList(SSI2DParamValue[]) - Constructor for class com.atid.lib.module.barcode.ssi.param.SSI2DParamValueList
  Create an instance of the SSI2DParamValueList class.
startDecode() - Method in class com.atid.lib.module.barcode.ATBarcode
  Instruct the instrument to read the bar code.
stop() - Method in class com.atid.lib.module.barcode.ATBarcode
  Instructs the Device to stop the operation being performed.
stop() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
stop() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Instructs the Device to stop the operation being performed.
StoredData() - Constructor for class com.atid.lib.reader.params.StoredDataList.StoredData
  Create an instance of StoredData
StoredData(DataType, String) - Constructor for class com.atid.lib.reader.params.StoredDataList.StoredData
  Create an instance of StoredData
StoredDataList - Class in com.atid.lib.reader.params
  The StoredDataList class is used to read or store data stored in the Device.
StoredDataList() - Constructor for class com.atid.lib.reader.params.StoredDataList
StoredDataList.StoredData - Class in com.atid.lib.reader.params
  The StoredData class is used by the StoredDataList class to represent each piece of data stored in the Device.
SymbolStateList - Class in com.atid.lib.module.barcode.params
  The SymbolStateList class is used to set or return symbol status to the barcode module.
SymbolStateList() - Constructor for class com.atid.lib.module.barcode.params.SymbolStateList
  Create an instance of the SymbolStateList class.

A B C D E F G H I K L M N O P Q R S T U V W