# Package com.atid.lib.module.rfid.uhf.types

- Enum Summary
  Enum | Description
  --- | ---
  AlgorithmType | The AlgorithmType enumeration represents the algorithm by which the RFID UHF module inventories the TAG.
  BankType | The BankType enumeration specifies the memory bank of the RFID UHF tag.
  GlobalBandType | The GlobalBandType enumeration represents the frequency direction of the RFID UHF module.
  LinkProfileType | Link Profile is an option to set the air interface method of RFID UHF
  Mask6cAction | The Mask6cAction enumeration type indicates the status of the Flag when the RFID UHF module performs the Inventory operation and the pattern of the given Selection Mask is set as the Target value of the Selection Mask according to the condition.
  Mask6cTarget | The Mask6cTarget enumeration represents the Flag where the result status of the Selection Mask will be saved when the RFID UHF module is inventoried.
  SelectFlag | The SelectFlag enumeration represents the status of the Select Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  SessionFlag | The SessionFlag enumeration type indicates the status of the Session Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.
  SessionTarget | The SessionTarget enumeration represents the Session Flag of the TAG to be the Inventory target when the RFID UHF module is running the Inventory.