A B C D E F G H I K L M N O P Q R S T U V W

## C

checkBufferSize(int) - Method in class com.atid.lib.transport.ATransport
CheckDigit - Enum in com.atid.lib.module.barcode.spc.type
  No Check Digit indicates that the scanner reads and transmits bar code data with or without a check digit.
checkError() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
checkError() - Method in class com.atid.lib.reader.ATEAReader
clear() - Method in class com.atid.lib.module.barcode.params.SymbolStateList
  Deletes all information in the SymbolStateList instance.
clear() - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Initializes the values ​​set in the SelectMask6cParam instance.
clearEpcMask() - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
clearEpcMask() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  Remove all EPC Mask items from the RFID UHF module of the device.
clearListener() - Method in class com.atid.lib.module.barcode.ATBarcode
  Removes all event handlers from the ATBarcode instance.
clearListener() - Method in class com.atid.lib.module.rfid.uhf.ATRfidUhf
  ATRfidUhf Removes all event handlers from the instance.
clearListener() - Method in class com.atid.lib.reader.ATEAReader
  Removes all listeners registered on an instance of the ATEAReader class.
CodabarCheckCharacter - Enum in com.atid.lib.module.barcode.spc.type
  Codabar check characters are created using different “modulos.”
CodabarConcatenation - Enum in com.atid.lib.module.barcode.spc.type
  Codabar supports symbol concatenation.
CodabarStartStopCharactersDetection - Enum in com.atid.lib.module.barcode.ssi.type
  Select whether to detect upper case or lower case Codabar start/stop characters.
Code11CheckDigitsRequired - Enum in com.atid.lib.module.barcode.spc.type
  This option sets whether 1 or 2 check digits are required with Code 11 bar codes.
Code11CheckDigitVerification - Enum in com.atid.lib.module.barcode.ssi.type
  This feature allows the decoder to check the integrity of all Code 11 symbols to verify that the data complies with the specified check digit algorithm.
Code39CheckCharacter - Enum in com.atid.lib.module.barcode.spc.type
  No Check Character indicates that the scanner reads and transmits bar code data with or without a check character.
CodeLength - Class in com.atid.lib.module.barcode.ssi.type
  The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
CodeLength() - Constructor for class com.atid.lib.module.barcode.ssi.type.CodeLength
CodeLength(int, int) - Constructor for class com.atid.lib.module.barcode.ssi.type.CodeLength
CodeLengthType - Enum in com.atid.lib.module.barcode.ssi.type
  The length of a code refers to the number of characters (i.e., human readable characters), including check digit(s) the code contains.
CodePages - Enum in com.atid.lib.module.barcode.spc.type
  ISO 2022/ISO 646 Character Replacements Code pages define the mapping of character codes to characters.
com.atid.lib.atx88 - package com.atid.lib.atx88
com.atid.lib.diagnostics - package com.atid.lib.diagnostics
com.atid.lib.module.barcode - package com.atid.lib.module.barcode
com.atid.lib.module.barcode.event - package com.atid.lib.module.barcode.event
com.atid.lib.module.barcode.params - package com.atid.lib.module.barcode.params
com.atid.lib.module.barcode.spc.param - package com.atid.lib.module.barcode.spc.param
com.atid.lib.module.barcode.spc.type - package com.atid.lib.module.barcode.spc.type
com.atid.lib.module.barcode.ssi.param - package com.atid.lib.module.barcode.ssi.param
com.atid.lib.module.barcode.ssi.type - package com.atid.lib.module.barcode.ssi.type
com.atid.lib.module.rfid.uhf - package com.atid.lib.module.rfid.uhf
com.atid.lib.module.rfid.uhf.atm - package com.atid.lib.module.rfid.uhf.atm
com.atid.lib.module.rfid.uhf.event - package com.atid.lib.module.rfid.uhf.event
com.atid.lib.module.rfid.uhf.params - package com.atid.lib.module.rfid.uhf.params
com.atid.lib.module.rfid.uhf.types - package com.atid.lib.module.rfid.uhf.types
com.atid.lib.reader - package com.atid.lib.reader
com.atid.lib.reader.event - package com.atid.lib.reader.event
com.atid.lib.reader.params - package com.atid.lib.reader.params
com.atid.lib.reader.types - package com.atid.lib.reader.types
com.atid.lib.transport - package com.atid.lib.transport
com.atid.lib.transport.types - package com.atid.lib.transport.types
com.atid.lib.types - package com.atid.lib.types
COMMAND_LENGTH - Static variable in enum com.atid.lib.module.barcode.spc.param.SPCParamName
CommType - Enum in com.atid.lib.reader.types
  ATEAReader Indicates the communication protocol of the instance and equipment.
CompositeBeepMode - Enum in com.atid.lib.module.barcode.ssi.type
  To select the number of decode beeps when a composite bar code is decoded, scan the appropriate bar code.
connect() - Method in class com.atid.lib.reader.ATEAReader
  An instance of the ATEAReader class tries to connect to the configured address
connect() - Method in class com.atid.lib.transport.ATransport
  Attempts to connect to the appliance using an instance of the Transport class.
connect() - Method in class com.atid.lib.transport.ATransportBluetooth
connect() - Method in class com.atid.lib.transport.ATransportBluetoothLe
connect() - Method in class com.atid.lib.transport.ATransportUsb
ConnectState - Enum in com.atid.lib.transport.types
  The ConnectState enumeration indicates the connection status of the ATransport instance.
ConnectType - Enum in com.atid.lib.transport.types
  The ConnectType enumeration indicates which communication method the ATransport instance uses in its connection with the appliance.
copy(SelectMask6cParam) - Method in class com.atid.lib.module.rfid.uhf.params.SelectMask6cParam
  Copy the SelectMask6cParam instance.
CouponReport - Enum in com.atid.lib.module.barcode.ssi.type
  Traditional coupon symbols (old coupon symbols) are composed of two bar codes: UPC/EAN and Code128.

A B C D E F G H I K L M N O P Q R S T U V W