A B C D E F G H I K L M N O P Q R S T U V W

## O

onAccessResult(ResultCode, ActionType, String, String, Object) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
onActionChanged(ResultCode, ActionType, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onBarcodeReadData(ATBarcode, BarcodeType, String, String, Object) - Method in interface com.atid.lib.module.barcode.event.IATBarcodeEventListener
  Invoked when the barcode module decodes the barcode.
onBatteryState(int, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onConnected(int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
onConnecting(int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
onDisconnected(int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
onDisonnecting(int) - Method in class com.atid.lib.transport.ATransportBluetoothLe
onEvent(int, byte[]) - Method in class com.atid.lib.atx88.ATx88Reader
onKeyEvent(KeyType, KeyState, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onNotificationState(NotificationState, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onOperationModeChanged(OperationMode, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onOverflow() - Method in interface com.atid.lib.transport.ATransport.IBufferControlEventListener
  Invoked when an overflow occurs in the Transport instance's internal buffer.
onPowerGainChanged(int, Object) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
onReaderActionChanged(ResultCode, ActionState, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderActionChanged(ATEAReader, ResultCode, ActionState, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  Called when the operational state of the Device associated with the ATEAReader instance changes.
onReaderBatteryState(int, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderBatteryState(ATEAReader, int, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  Called to report the battery state of the Device attached to the ATEAReader instance before it occurs.
onReaderKeyChanged(KeyType, KeyState, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderKeyChanged(ATEAReader, KeyType, KeyState, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  Called to report the key type and state of the Device attached to the ATEAReader instance before it occurs.
onReaderNotificationState(NotificationState, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderOperationModeChanged(OperationMode, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderOperationModeChanged(ATEAReader, OperationMode, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  Invoked when the Operation Mode of the Device attached to the ATEAReader instance changes.
onReaderStateChanged(ConnectState, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderStateChanged(ATEAReader, ConnectState, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  The ATransport instance associated with the ATEAReader instance is called when the connection state of the Device changes.
onReaderUsbChargerChanged(UsbChargerType, UsbChargerState, Object) - Method in class com.atid.lib.reader.ATEAReader
onReaderUsbChargerChanged(ATEAReader, UsbChargerType, UsbChargerState, Object) - Method in interface com.atid.lib.reader.event.IATEAReaderEventListener
  Called to report the USB type and state of the Device attached to the ATEAReader instance before it occurs.
onReadTag(String, Object) - Method in class com.atid.lib.module.rfid.uhf.atm.ATRfidUhfATM
onReceivedData(byte[]) - Method in class com.atid.lib.transport.ATransportBluetoothLe
onRfidUhfAccessResult(ATRfidUhf, ResultCode, ActionState, String, String, Object) - Method in interface com.atid.lib.module.rfid.uhf.event.IATRfidUhfEventListener
  It is called when the device receives the result of executing the functions of Read Memory, Write Memory, Lock and so on.
onRfidUhfPowerGainChanged(ATRfidUhf, int, Object) - Method in interface com.atid.lib.module.rfid.uhf.event.IATRfidUhfEventListener
  Invoked when the Power Gain is changed on the Device.
onRfidUhfReadTag(ATRfidUhf, String, Object) - Method in interface com.atid.lib.module.rfid.uhf.event.IATRfidUhfEventListener
  Called when the device reads the tag while performing the Inventory function.
onStateChanged(ConnectState, Object) - Method in class com.atid.lib.atx88.ATx88Reader
onStateChanged(ConnectState, Object) - Method in class com.atid.lib.reader.ATEAReader
onStateChanged(ConnectState, Object) - Method in interface com.atid.lib.transport.ATransport.IConnectStateEventListener
  Called when the connection state of the ATransport instance and the device changes.
onUnderflow() - Method in interface com.atid.lib.transport.ATransport.IBufferControlEventListener
  Invoked when an underflow occurs in the Transport instance's internal buffer.
onUsbChargerChanged(UsbChargerType, UsbChargerState, Object) - Method in class com.atid.lib.atx88.ATx88Reader
OperationMode - Enum in com.atid.lib.reader.types
  The OperationMode enumeration type represents the Device's Operation Mode.

A B C D E F G H I K L M N O P Q R S T U V W