Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X

## G

G2TARGET_A - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
G2TARGET_AB - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
G2TARGET_B - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
GLOBAL_SCROLL - Static variable in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Specifies an acquire mode of "Global Scroll".
g2Erase(int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Erases (fills with zeros) data in a Class1/Gen2 tag.
g2Read(int, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs a low-level read of data from the Class1/Gen2 tag.
g2Wake(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Causes the reader to issue a number of G2 Select commands, in order to return tags in the field back to the "not inventoried" state.
g2Wake() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Causes the reader to issue a single G2 Select command, in order to return tags in the field back to the "not inventoried" state.
g2Write(int, int, byte[], int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs a low-level write of data to a Class1/Gen2 tag, at an arbitrary memory bank and location.
generateCRC16Checksum09(byte[], int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Generates a CRC-type checksum used to store an EPC-64 ID.
generateCRC16Checksum10(byte[], int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Generates a CRC-type checksum used to store an EPC-64 ID.
generateCRC16Checksum10(String) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Generates a CRC-type checksum for a Tag ID string.
generateLRC16Checksum(byte[], int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Generates an LRC16-type checksum over a portion of a byteArray.
getAcqC1Mask() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
getAcqG2AccessPwd() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the Access password that the reader will use to gain access to password-protected portions of Class1/Gen2 tag memory.
getAcqG2Mask() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current tag Class1/Gen2 mask, as a String.
getAcqG2MaskAction() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current include/exclude behavior of the Class1/Gen2 mask.
getAcqG2MaskAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current value of AcqG2MaskAntenna.
getAcqG2SL() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current value of AcqG2SL.
getAcqMask() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
getAcquireC0Count() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of reads to perform in each Class0 acquire cycle.
getAcquireC0Cycles() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of complete acquire cycles to perform with each Class0 read operation.
getAcquireC1Count() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as getAcquireCount().
getAcquireC1Count() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of reads to perform in each C1 acquire cycle.
getAcquireC1Cycles() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as getAcquireCycles().
getAcquireC1Cycles() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of complete acquire cycles to perform with each C1 read operation.
getAcquireC1EnterWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as getAcquireEnterWakeCount().
getAcquireC1EnterWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of wakes to perform at the start of each C1 acquire cycle.
getAcquireC1ExitWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as getAcquireExitWakeCount().
getAcquireC1ExitWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of wakes to perform at the end of each C1 acquire cycle.
getAcquireC1SleepCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Performs the same task as getAcquireSleepCount().
getAcquireC1SleepCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of sleeps to perform after each C1 acquire cycle.
getAcquireCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of reads to perform in each Class1 Gen1 acquire cycle.
getAcquireCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getAcquireCycles() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of complete acquire cycles to perform with each Class1 Gen1 read operation.
getAcquireCycles() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getAcquireEnterWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of wakes to perform at the start of each Class1 Gen1 acquire cycle.
getAcquireEnterWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getAcquireExitWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of wakes to perform at the end of all the Class1 Gen1 acquire cycles.
getAcquireExitWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getAcquireG2Count() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of reads to perform in each Class1 Gen2 acquire cycle.
getAcquireG2Count() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of reads to perform in each G2 acquire cycle.
getAcquireG2Cycles() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of complete acquire cycles to perform with each Class1 Gen2 read operation.
getAcquireG2Cycles() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of complete acquire cycles to perform with each G2 read operation.
getAcquireG2Ops() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
getAcquireG2Ops(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
getAcquireG2OpsMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of AcqG2OpsMode.
getAcquireG2Q() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the starting Q value to use in each Class1 Gen2 acquire cycle.
getAcquireG2Q() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the starting Q value for each G2 acquire cycle.
getAcquireG2Selects() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of SELECT commands issued at the start of each Class1/Gen2 acquire cycle.
getAcquireG2Session() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the G2 Session that the reader will operate on when inventorying Class1/Gen2 tags.
getAcquireG2TagData() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns a String specifying which additional locations in G2 tag memory to fetch in the course of an inventory.
getAcquireG2Target() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the String which specifies the manner in which the reader manages the population of inventoried G2 tags.
getAcquireMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the method that the reader uses to scan for tags.
getAcquireMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the method that the reader uses to scan for tags.
getAcquireMode() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the method that the reader uses to scan for tags.
getAcquireSleep() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF AcquireSleep state, which specifies whether tags are slept as they are read.
getAcquireSleepCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of sleeps to perform after each Class1 Gen1 acquire cycle.
getAcquireSleepCount() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getAcquireTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum inventory duration, after which the reader aborts the inventory.
getAcquireWakeCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of acquire events the reader will perform in between issuing Wakes.
getActionListener() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Returns the object that has been registered by this `SerialDiscoveryListenerService` to receive messages about the progress of the serial port scanning.
getActiveAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the number of the active antenna.
getActiveAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of the active antenna.
getAddress() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns a human-friendly string describing the reader's address.
getAntenna() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the antenna that this Tag was last seen with.
getAntennaSequence() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the Antenna Sequence, as a comma-separated String of hex values.
getAntennaSequence() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Return the sequence of antenna ports the reader cycles through as it performs reads.
getAntennaSequence() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the Antenna Sequence, as a comma-separated String of hex values.
getAntennaStatus() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the Antenna Status.
getAutoAction() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the action the reader performs while in autonomous mode.
getAutoErrorOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader setting specifying which AutoMode errors to react to, and the external output setting to apply when one of those errors is encountered.
getAutoFalseOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value of the external output pins while in the "false pause" state.
getAutoFalsePause() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time the reader pauses after the autonomous mode evaluation returns a `false` condition.
getAutoMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the ON/OFF status of Autonomous mode.
getAutoMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of Autonomous mode.
getAutoMode() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the ON/OFF status of Autonomous mode.
getAutoModeStatus() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns a value representing the current state of autonomous mode state machine.
getAutoProgError() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the antenna value reported by the reader when a programming attempt in AutoMode fails.
getAutoStartPause() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time the reader pauses after receiving a start trigger before it actually enters the work state.
getAutoStartTrigger() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the external input pins the reader monitors that trigger autonomous mode to jump into the working state.
getAutoStopPause() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time the reader pauses after receiving a stop trigger before it actually leaves the work state.
getAutoStopTimer() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time the reader spends in the work state before moving on to the evaluate state.
getAutoStopTrigger() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the external input pins the reader monitors that trigger autonomous mode to leave the working state.
getAutoTrueOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value of the external output pins while in the "true pause" state.
getAutoTruePause() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time the reader pauses after the autonomous mode evaluation returns a `true` condition.
getAutoWaitOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value of the external output pins while in the wait state.
getAutoWorkOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value of the external output pins while in the work state.
getAvailableBaudRates() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap denoting the available baud rates for this reader.
getBank() - Method in class com.alien.enterpriseRFID.reader.TagMemory
getBaudRate() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the reader's serial communication baud rate.
getBidirectionalDDR() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap defining the direction of the Bi-Directional I/O ports.
getBidirectionalIOPorts() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap specifying which of the I/O ports have been configured to be Bidirectional inputs/outputs.
getBitArray(byte[]) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Returns an array of bits, given an array of bytes.
getBitArray(byte[], int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Get Bit Array from an array of bytes, specifying the offset and length to extract data from within the byte array.
getByteArray(byte[]) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Get an array of bytes from an array of bits.
getCRC() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns this Tag's CRC as a long integer.
getCommandPort() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the port number that this DiscoveryItem's reader uses to accept and respond to host commands over the network.
getCommandPort() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the port number that this reader listens on for command messages.
getConnection() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the connection method of the reader represented by this DiscoveryItem.
getCustomFormatString() - Static method in class com.alien.enterpriseRFID.tags.TagUtil
getCustomTagList(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags a specified number of times and reports the results.
getCustomTagList() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags once and reports the results.
getDHCP() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of DHCP.
getDNS() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the Domain Name Server for this reader.
getData() - Method in class com.alien.enterpriseRFID.reader.TagMemory
getDate() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the Date of this Message.
getDebugLevel() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the current Debug Level setting.
getDirection() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the apparent direction of the tag, toward or away from the antenna.
getDiscoverTime() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the discovery time of this Tag, as reported by the reader.
getDiscoveryItems() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Returns an array of `DiscoveryItem`s representing all of the readers that this `NetworkDiscoveryListenerService` knows about.
getDiscoveryItems() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Returns an array of `DiscoveryItem`s representing all of the readers that this `SerialDiscoveryListenerService` knows about.
getDiscoveryListener() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Returns the object that has been registered by this `NetworkDiscoveryListenerService` to receive messages when readers are discovered, renewed, or removed from the network.
getDiscoveryListener() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Returns the object that has been registered by this `SerialDiscoveryListenerService` to receive messages when readers are discovered, renewed, or removed on the serial ports.
getDiscoveryMethod() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the method with which this DiscoveryItem's reader was discovered.
getEventTime() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Returns the timestamp of this ExternalIO event, as reported by the reader's on-board clock.
getEventTimeHost() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Returns the timestamp of this ExternalIO event, as reported by the host system's clock.
getExternalInput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the decimal representation of the state of the external inputs.
getExternalInput() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the decimal representation of the state of the external inputs.
getExternalOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the decimal representation of the state of the external outputs.
getFirstHeartbeat() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the time that this DiscoveryItem first registered a heartbeat signal from its reader.
getG2Data(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns a chunk of additional Gen2 tag data, as a String.
getG2Data() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns all of the additional Gen2 tag data, as an array of Strings.
getG2Ops(int) - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns a result from a specific G2Ops action, as a String.
getG2Ops() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns all of the result codes for the G2Ops actions, as an array of Strings.
getGateway() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the IP address of the network Gateway server.
getGeneralPurposeInputs() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap specifying which of the I/O ports have been configured to be General Purpose Inputs.
getGeneralPurposeOutputs() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap specifying which of the I/O ports have been configured to be General Purpose Outputs.
getHardwareReaderType() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns this reader's Reader Type.
getHashtable() - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Returns the Hashtable that this XMLWriter uses to generate its XML document.
getHeartbeatAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the IP address where reader heartbeat messages are delivered.
getHeartbeatCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of heartbeat messages that the reader will broadcast following startup.
getHeartbeatPort() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the port number over which the reader sends its UDP heartbeat messages.
getHeartbeatTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time interval between heartbeat messages.
getHopInterval() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the length of time the reader dwells at each frequency before hopping to the next one.
getHopStepSize() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the frequency spacing of this reader's hop table.
getHostDiscoverTime() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the discovery time of this Tag, as reported by the host.
getHostRenewTime() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the time this Tag was last seen, as reported by the host.
getHostname() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the network hostname for this reader.
getIO(int) - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the `ExternalIO` that holds position `index` in this `Message`'s IOList.
getIOCount() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the number of ExternalIOs in this `Message`'s IOList.
getIOList() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the IOList of this notification message, as an array of `ExternalIO`s.
getIOList() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Asks the reader for its current IOList and reports the results.
getIOListCustomFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current custom IOList formatting string.
getIOListDump() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns a single dump of the reader's current IOList.
getIOListFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current format for IOLists.
getIOPortValue() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the current state of the input/output port pins.
getIOStreamAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the address of the device to push IOStream events to.
getIOStreamCustomFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current custom IOStream formatting string.
getIOStreamFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of format used for IOStream event messages.
getIOStreamKeepAliveTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time period (in seconds) the reader will hold an idle IOStream TCP socket open before closing it.
getIOStreamMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the the reader's IOStream functionality.
getIOType() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of external I/Os that the reader will report from its internal IOList.
getIPAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the configured IP Address of this reader.
getIndentSize() - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Returns the number of space characters used to indent each level of XML output.
getInfo() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's information dump, which includes all of the current reader settings.
getInitExternalOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value used to set the external output state during startup.
getInputStream() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the InputStream that is used to receive replies from the reader.
getInputStream() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the InputStream object for the serial port managed by this SerialManager.
getInvertExternalInput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the external input inverter.
getInvertExternalOutput() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the external output inverter.
getLBT() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of LBT.
getLBTLimit() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current setting for the LBT threshold.
getLBTValue() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current wide-band noise level that the reader is detecting.
getLastHeartbeat() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the time that this DiscoveryItem last registered a heartbeat signal from its reader.
getLeaseTime() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the amount of time the reader represented by this DiscoveryItem waits between sending its heartbeat messages across the network.
getLen() - Method in class com.alien.enterpriseRFID.reader.TagMemory
getLineTerminator() - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Returns the line terminator string that this XMLWriter uses to end each of the lines of its XML output.
getListenerInterface() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Returns the interface IP address that this `MessageListenerService` is listening on for reader notification messages.
getListenerPort() - Method in class com.alien.enterpriseRFID.discovery.NetworkDiscoveryListenerService
  Returns the port number for this service to listen on.
getListenerPort() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Returns the port number that this `MessageListenerService` is listening on for reader notification messages.
getLocalizationCode() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns this reader's Localization Code.
getLoggingInterval(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns the periodicity at which the tag logs sensor data to tag memory, with timing values returned as a triple byte array.
getMACAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's MAC address.
getMailFrom() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the email address associated with this reader.
getMailServer() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the SMTP (Simple Mail Transfer Protocol) mail server.
getMask() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Deprecated. Current readers only support AcqG2Mask.
getMask() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the current tag mask.
getMaxAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum antenna port number that this reader's hardware supports.
getMaxAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the maximum antenna number that may be addressed by this reader.
getMaxFrequency() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the maximum RF frequency that this reader may be set to.
getMaxHopTableIndex() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the maximum allowable Hop Channel that is used in the hopping table.
getMaxRFChannel() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the maximum RF channel used in this reader.
getMaxRFPower() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the maximum RF power available with this reader hardware.
getMaxSerialPort() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Deprecated. use `SerialDiscoveryListenerService.getSerialPortList()` instead
getMemory(String, int, int) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns a chunk of tag memory from the specified tag.
getMemoryPacketSize() - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns the number of bytes to use in each memory related transmission packet to and from the tag.
getMessageListener() - Method in class com.alien.enterpriseRFID.notify.MessageListenerService
  Returns the `MessageListener` object that has been registered by this `MessageListenerService` to be notified when reader notifications arrive.
getMinFrequency() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the minimum RF frequency that this reader may be set to.
getMyData() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the arbitrary "MyData" stored on the reader.
getNetmask() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the netmask of this reader.
getNetworkTimeout() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time period (in seconds) the reader will wait on an idle network connection before timing out.
getNetworkUpgrade() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the network upgrade flag.
getNotifyAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the address of the device to push notifications to.
getNotifyFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of format used for notification messages.
getNotifyHeader() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of NotifyHeader.
getNotifyInclude() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the value indicating whether Tag data, I/O data, or both will be included in Notification messages.
getNotifyKeepAliveTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time period (in seconds) the reader will hold an idle Notify TCP socket open before closing it.
getNotifyMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of Notify mode.
getNotifyQueueLimit() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the total number of failed TCP notification messages that the reader will queue up, waiting for the connection to the NotifyAddress to be reestablished.
getNotifyRetryCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of times the reader should retry a notification message that failed to be delivered, before turning NotifyMode off.
getNotifyRetryPause() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the amount of time (in seconds) that the reader should retry wait before reattempting a failed notification message.
getNotifyTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time interval for automatic pushing of tag lists.
getNotifyTrigger() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the event conditions (other than time-based) upon which a notification message is sent out to any listener.
getOperatingVoltage() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the measured voltage level into the OEM Module, given in hundredths of a volt.
getOutputStream() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Get the OutputStream as a OutputStream
getOutputStream() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the OutputStream object for the serial port managed by this SerialManager.
getPCWord() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns information about a tag's Protocol Control (PC) information.
getPLLType() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the type of PLL installed in this reader.
getPassword() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the password associated with this DiscoveryItem's reader.
getPassword() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the password that this `AlienClass1Reader` uses to authenticate with a reader via the network.
getPersistTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the time, in seconds, that tags on the internal TagList will persist without having been read, before being purged from the list.
getPersistTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the length of time a read tag will remain in the reader's internal list of active tags.
getPersistTime() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the time, in seconds, that tags on the internal TagList will persist without having been read, before being purged from the list.
getPersistTime() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the PersistTime associated with this Tag.
getPersistTime() - Method in class com.alien.enterpriseRFID.tags.TagTable
  Returns this TagTable's persistence time.
getProgAlienImageMap() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current memory map specifier used by the ProgramAlienImage command.
getProgAlienImageNSI() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the NSI data that the reader will write to the tag during the next ProgramAlienImage.
getProgAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the number of the programming antenna.
getProgAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the antenna that the reader uses for programming operations.
getProgAntenna() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the number of the programming antenna.
getProgAttempts() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of times the reader attempts to program a tag.
getProgBlockAlign() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current ON/OFF status of ProgBlockAlign.
getProgBlockSize() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current ProgBlockSize value.
getProgC1KillPwd() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the kill password that the reader will use to lock or kill the next Class 1, Gen 1 tag while operating in AutoMode.
getProgDataUnit() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the size of the data unit used to read and write to Gen2 tags.
getProgEPCData() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the EPC data that the reader will use to program the next tag in AutoMode, or when the ProgramEPC command is issued without a corresponding EPC data argument.
getProgEPCDataInc() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the programming result that triggers the ProgEPCData property of the reader to be incremented.
getProgEPCDataIncCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum number of times the reader will automatically increment the ProgEPCData value before prohibiting further programming operations.
getProgEraseAttempts() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of times the reader attempts to erase a tag, before programming it.
getProgG2AccessPwd() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the Access Password that the reader will use when the ProgramAccessPwd command is issued without a corresponding data argument.
getProgG2KillPwd() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the kill password that the reader will use to lock or kill the next Class 1, Gen 2 tag while operating in AutoMode.
getProgG2LockType() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of lock used to lock the next Class1/Gen2 tag.
getProgG2NSI() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the NSI data that the reader will write to the tag during the next ProgramEPC operation.
getProgIncrementOnFail() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the ProgIncrementOnFail flag.
getProgProtocol() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the tag protocol that the reader is using for programming operations.
getProgReadAttempts() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the number of times the reader attempts to verify the presence of a tag, before programming it.
getProgSingulate() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of whether the reader will try to singulate a tag before programming it.
getProgUserData() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the USER data that the reader will use when the ProgramUser command is issued without a corresponding data argument.
getProgUserDataInc() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the programming result that triggers the ProgUserData property of the reader to be incremented.
getProgUserDataIncCount() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the maximum number of times the reader will automatically increment the ProgUserData value before prohibiting further programming operations.
getProgramEnableMode() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns a bitmap specifying which program functions are enabled for this reader.
getProgramID() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the tagID the reader will use to program the next tag in AutoMode.
getProgramPassCode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the kill password that the reader will use to lock or kill the next Class 1, Gen 1 tag while operating in AutoMode.
getProtocol() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the protocol code for this tag.
getProtocolString() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the protocol string for this tag.
getProtocolString(int) - Static method in class com.alien.enterpriseRFID.tags.Tag
  Returns the protocol string associated with the given protocol code.
getPtr() - Method in class com.alien.enterpriseRFID.reader.TagMemory
getRFAttenuation() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFAttenuation value.
getRFAttenuation(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFAttenuation value for the given antenna.
getRFAttenuation() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the RF power attenuation value from non-volatile memory.
getRFAttenuations() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFAttenuation values for reading tags and writing tags.
getRFAttenuations(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFAttenuation values for a specific antenna for reading tags and writing tags.
getRFChannel() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the RF channel currently being used by this reader.
getRFLevel() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFLevel value.
getRFLevel(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFLevel value for a specific antenna.
getRFLevels() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFLevel values for reading tags and writing tags.
getRFLevels(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's RFLevel values for a specific antenna for reading tags and writing tags.
getRFModulation() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's current Class 1 Gen2 modulation mode.
getRFOnOff() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the current state of the RF power while the reader is idle.
getRSSI() - Method in class com.alien.enterpriseRFID.tags.Tag
  Gets the last RSSI measurement for this tag.
getRSSIFilter() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the String defining the current RSSIFilter ranges.
getRadioType() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the type of RF radio in this reader.
getRawData() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the raw data content of the notification message sent by the reader.
getReader() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Instantiates a new `AlienClass1Reader` object, based on the attributes of this DiscoveryItem.
getReaderAddress() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the address of the reader represented by this DiscoveryItem.
getReaderBaudRate() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's current serial baud rate.
getReaderCommandPort() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the Command port number of the reader as indicated in the reader's notification message.
getReaderFunction() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's current operating mode.
getReaderHostname() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the network hostname of the reader as indicated in the reader's notification message.
getReaderIPAddress() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the IP Address of the reader as indicated in the reader's notification message.
getReaderMACAddress() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the MAC address of the reader represented by this DiscoveryItem.
getReaderMACAddress() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the MAC Address of the reader as indicated in the reader's notification message.
getReaderName() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns this DiscoveryItem's ReaderName value.
getReaderName() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the name of the reader as indicated in the reader's notification message.
getReaderName() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the reader name.
getReaderName() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's Name.
getReaderName() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the reader name.
getReaderNumber() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's numerical identifier.
getReaderNumber() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the ReaderNumber stored in this reader.
getReaderPassword() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the password stored in the reader that is used to authenticate users attempting to access this reader via the network.
getReaderReply() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the full contents of the reader's most recent reply, which generally takes the form of a "keyword=value" phrase.
getReaderReplyKeyword() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the "keyword" portion of the reader's most recent reply.
getReaderReplyValueInt() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the "value" portion of the reader's most recent reply, parsed as an int.
getReaderReplyValueString() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the "value" portion of the reader's most recent reply, parsed as a String.
getReaderSerialNumber() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
getReaderType() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns this DiscoveryItem's ReaderType value.
getReaderType() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the type of the reader as indicated in the reader's notification message.
getReaderType() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the reader type.
getReaderType() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns a string describing the type of reader.
getReaderType() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the reader type.
getReaderUsername() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the username stored in the reader that is used to authenticate users attempting to access this reader via the network.
getReaderVersion() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns this DiscoveryItem's ReaderVersion value.
getReaderVersion() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the firmware version of this reader.
getReaderVersion() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns a string describing the version of the reader.
getReaderVersion() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the firmware version of this reader, including the ReaderLocale and ReaderType values.
getReason() - Method in class com.alien.enterpriseRFID.notify.Message
  Gets the Reason value for this Message.
getReceiveAntenna() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the receive antenna that this Tag was last seen with.
getRenewCount() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the number of times this Tag has been read.
getRenewTime() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the time this Tag was last seen be the reader.
getSensorValue(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns the sensor value of the tag's onboard sensor.
getSerialBaudRate() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Returns the serial baud rate used to discover serially-connected readers.
getSerialBaudRate() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the communication rate of the serial port managed by this SerialManager.
getSerialPort() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the SerialPort object managed by this SerialManager.
getSerialPort(String) - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns a SerialPort object associated with the given serialPortName.
getSerialPortList() - Method in class com.alien.enterpriseRFID.discovery.SerialDiscoveryListenerService
  Returns the list of serial ports that will be scanned.
getSerialPortList() - Static method in class com.alien.enterpriseRFID.util.SerialManager
  Returns a list of available serial ports on this host.
getSerialPortName() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the name of the serial port managed by this SerialManager.
getSerialPortTimeout() - Method in class com.alien.enterpriseRFID.util.SerialManager
  Returns the communication timeout value for the serial port managed by this SerialManager.
getSmoothPosition() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the tag's position, relative to its first read.
getSmoothSpeed() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the averaged/smoothed speed of this tag.
getSocket(InetAddress, int, int) - Static method in class com.alien.enterpriseRFID.reader.TimedSocket
  Attempts to connect to a service at the specified address and port, for a specified maximum amount of time.
getSocket(String, int, int) - Static method in class com.alien.enterpriseRFID.reader.TimedSocket
  Attempts to connect to a service at the specified address and port, for a specified maximum amount of time.
getSpeed() - Method in class com.alien.enterpriseRFID.tags.Tag
  Gets the last speed measurement for this tag.
getSpeedFilter() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the String defining the current SpeedFilter ranges.
getSpeedSmoothingCoefficient() - Static method in class com.alien.enterpriseRFID.tags.Tag
  Returns the current speed smoothing coeefficient.
getStartTriggerLines() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the external input lines that triggered this autonomous cycle to start.
getStopTriggerLines() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the external input lines that triggered this autonomous cycle to stop.
getStreamHeader() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the StreamHeader.
getSupportedTagTypes() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the bitmap indicating which Alien RFID tag types the reader should look for.
getTag(int) - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the `Tag` that holds position `index` in this `Message`'s `TagList`.
getTag() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Acquires one Tag, once.
getTag(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Acquires one Tag, using a multiplier.
getTag(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags a specified number of times and reports the first tag.
getTag() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags once and reports the results the first tag.
getTag() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Acquires one Tag, once.
getTag(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Acquires one Tag, using a multiplier.
getTagAuth() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current TagAuth setting on the reader.
getTagAuth() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns information about tag authentication.
getTagCount() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the number of tags in this `Message`'s TagList.
getTagID() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Acquires tags, and returns the TagID of the first tag on the TagList.
getTagID(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags a specified number of times and reports the ID of the first tag.
getTagID() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags once and reports the ID of the first tag.
getTagID(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns the ID of a unique tag specified by the mask commands.
getTagID() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Acquires tags, and returns the TagID of the first tag on the TagList.
getTagID() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns this Tag's TagID attribute.
getTagInfo() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  The TagInfo command returns low-level information about a tag, such as the manufacturer ID, tag model and version.
getTagInfo(String) - Method in class com.alien.enterpriseRFID.reader.AlienClassBPTReader
  Returns information about a single tag being masked.
getTagList() - Method in class com.alien.enterpriseRFID.notify.Message
  Returns the TagList of this notification message, as an array of `Tag`s.
getTagList() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns an array of tags known to the reader, once.
getTagList(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Fetches and returns the tag list, using a multiplier count.
getTagList(long) - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Reads tags for the specified number of milliseconds.
getTagList(int) - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags a specified number of times and reports the results.
getTagList() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Immediately scans the field for tags once and reports the results.
getTagList() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns an array of tags known to the reader, once.
getTagList(int) - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Fetches and returns the tag list, using a multiplier count.
getTagList() - Method in class com.alien.enterpriseRFID.tags.TagTable
  Returns the list of tags in this TagTable, as an array of Tag objects.
getTagListAntennaCombine() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of TagList Antenna Combine feature.
getTagListCustomFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current printf-style custom tag list formatting string.
getTagListFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current format for tag lists.
getTagListMillis() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of TagList Milliseconds feature.
getTagStreamAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the address of the device to push TagStream events to.
getTagStreamCountFilter() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the minimum and maximum values for the TagStreamCountFilter, as the first two elements of an int[].
getTagStreamCountFilterMinimum() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the minimum number of times a given tag has to be read before the reader will start streaming that tag data.
getTagStreamCustomFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the current custom TagStream formatting string.
getTagStreamFormat() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the type of format used for TagStream event messages.
getTagStreamKeepAliveTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the time period (in seconds) the reader will hold an idle TagStream TCP socket open before closing it.
getTagStreamMode() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the ON/OFF status of the the reader's TagStream functionality.
getTagTableListener() - Method in class com.alien.enterpriseRFID.tags.TagTable
  Returns the `TagTableListener` that has been registered with this TagTable to receive notifications when the tag list changes.
getTagType() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  High Level functions
getTagType() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the bitmap indicating which Alien RFID tag types the reader should look for.
getTime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the date and time of the reader's onboard clock, as a `Date` object.
getTimeOutMilliseconds() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
  Returns the maximum time to wait for a reader's reply, in milliseconds.
getTimeOutMode() - Method in class com.alien.enterpriseRFID.reader.AbstractReader
getTimeServer() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the address of the external TimeServer the reader uses to accurately set its internal clock each time it is rebooted.
getTimeToLive() - Method in class com.alien.enterpriseRFID.tags.Tag
  Calculates and returns this Tag's TimeToLive value.
getTimeZone() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the reader's time zone setting.
getTimer() - Method in class com.alien.enterpriseRFID.reader.AlienClass01Reader
  Returns the Timer text for the most recent acquire.
getTimer() - Method in class com.alien.enterpriseRFID.reader.AlienClassOEMReader
  Returns the Timer text for the most recent acquire.
getTopLevelTag() - Method in class com.alien.enterpriseRFID.util.XMLWriter
  Returns the top-level tag string that this XML writer wraps around its XML output.
getTransmitAntenna() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns the transmit antenna that this Tag was last seen with.
getType() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Returns this ExternalIO's type.
getTypeString() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Returns this ExternalIO's type, as a string.
getUpgradeAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the URL where the reader will look for upgrade files.
getUpgradeIPAddress() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the IP address for the Reader Upgrade Service (RUS) where the reader will look for upgrade files.
getUpgradePort() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the port number for the Reader Upgrade Service (RUS) that the reader will connect to when it looks for upgrades over the network.
getUptime() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the elapsed time, in seconds, since the last time the reader was rebooted.
getUsername() - Method in class com.alien.enterpriseRFID.discovery.DiscoveryItem
  Returns the username associated with this DiscoveryItem's reader.
getUsername() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the username that this `AlienClass1Reader` uses to authenticate with a reader via the network.
getValue() - Method in class com.alien.enterpriseRFID.externalio.ExternalIO
  Returns the value for this ExternalIO.
getValue(byte[], int, int) - Static method in class com.alien.enterpriseRFID.util.BitMath
  Return a long value from a bit array.
getWWWPort() - Method in class com.alien.enterpriseRFID.reader.AlienClass1Reader
  Returns the port number that the reader's built-in web server listens on.
getXML() - Method in class com.alien.enterpriseRFID.notify.Message
  Deprecated. Use `Message.getRawData()` instead.
getXMLString() - Method in class com.alien.enterpriseRFID.util.XMLReader
  Returns the XML string data being parsed.
getXPC() - Method in class com.alien.enterpriseRFID.tags.Tag
  Returns information about a tag's Extended Protocol Control (XPC) information.
getZeroSpeedThresholdHigh() - Static method in class com.alien.enterpriseRFID.tags.Tag
  Returns the current high end of the zero-speed threshold.
getZeroSpeedThresholdLow() - Static method in class com.alien.enterpriseRFID.tags.Tag
  Returns the current low end of the zero-speed threshold.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I K L M N O P R S T U V W X